#include "bcm6358.dtsi"

#include <dt-bindings/input/input.h>

/ {
	model = "BT Home Hub 2.0 Type A";
	compatible = "bt,home-hub-2-a", "brcm,bcm6358";

	aliases {
		led-boot = &led_power_green;
		led-failsafe = &led_power_green;
		led-running = &led_power_green;
		led-upgrade = &led_upgrading_green;
	};

	chosen {
		bootargs = "rootfstype=squashfs,jffs2 noinitrd console=ttyS0,115200";
		stdout-path = "serial0:115200n8";
	};

	keys {
		compatible = "gpio-keys-polled";
		#address-cells = <1>;
		#size-cells = <0>;
		poll-interval = <20>;

		phone {
			label = "phone";
			gpios = <&pinctrl 1 1>;
			linux,code = <KEY_PHONE>;
			debounce-interval = <60>;
		};

		reset {
			label = "reset";
			gpios = <&pinctrl 9 1>;
			linux,code = <KEY_RESTART>;
			debounce-interval = <60>;
		};

		wps {
			label = "wps";
			gpios = <&pinctrl 11 1>;
			linux,code = <KEY_WPS_BUTTON>;
			debounce-interval = <60>;
		};
	};
};

&leds {
	status = "okay";

	pinctrl-names = "default";
	pinctrl-0 = <&pinctrl_serial_led>;

	led@0 {
		reg = <0>;
		active-low;
		label = "red:power";
	};

	led_power_green: led@1 {
		reg = <0>;
		active-low;
		label = "green:power";
		default-state = "on";
	};

	led@2 {
		reg = <2>;
		active-low;
		label = "blue:power";
	};

	led@3 {
		reg = <3>;
		active-low;
		label = "red:broadband";
	};

	led@4 {
		reg = <4>;
		active-low;
		label = "green:broadband";
	};

	led@5 {
		reg = <5>;
		active-low;
		label = "blue:broadband";
	};

	led@6 {
		reg = <6>;
		active-low;
		label = "red:wireless";
	};

	led@7 {
		reg = <7>;
		active-low;
		label = "green:wireless";
	};

	led@8 {
		reg = <8>;
		active-low;
		label = "blue:wireless";
	};

	led@9 {
		reg = <9>;
		active-low;
		label = "red:phone";
	};

	led@10 {
		reg = <10>;
		active-low;
		label = "green:phone";
	};

	led@11 {
		reg = <11>;
		active-low;
		label = "blue:phone";
	};

	led@12 {
		reg = <12>;
		active-low;
		label = "red:upgrading";
	};

	led_upgrading_green: led@13 {
		reg = <13>;
		active-low;
		label = "green:upgrading";
	};

	led@14 {
		reg = <14>;
		active-low;
		label = "blue:upgrading";
	};
};

&pflash {
	status = "okay";

	partitions {
		compatible = "fixed-partitions";
		#address-cells = <1>;
		#size-cells = <1>;

		cfe@0 {
			label = "CFE";
			reg = <0x000000 0x020000>;
		};

		linux@20000 {
			label = "linux";
			reg = <0x020000 0xfc0000>;
			compatible = "brcm,bcm963xx-imagetag";
		};

		nvram@fe0000 {
			label = "nvram";
			reg = <0xfe0000 0x020000>;
		};
	};
};

&uart0 {
	status = "okay";
};
