// SPDX-License-Identifier: GPL-2.0-or-later OR MIT

#include "ar9344.dtsi"

#include <dt-bindings/gpio/gpio.h>
#include <dt-bindings/input/input.h>

/ {
	model = "Sitecom WLR-7100 (X7 AC1200)";
	compatible = "sitecom,wlr-7100", "qca,ar9344";

	aliases {
		led-boot = &led_power;
		led-failsafe = &led_power;
		led-running = &led_power;
		led-upgrade = &led_power;
	};

	keys {
		compatible = "gpio-keys";

		wlan2g {
			label = "2.4GHz";
			gpios = <&gpio 16 GPIO_ACTIVE_LOW>;
			linux,code = <KEY_RESTART>;
		};

		wlan5g {
			label = "5GHz";
			gpios = <&gpio 15 GPIO_ACTIVE_LOW>;
			linux,code = <KEY_WPS_BUTTON>;
		};
	};

	leds {
		compatible = "gpio-leds";

		ops {
			label = "white:ops";
			gpios = <&gpio 12 GPIO_ACTIVE_LOW>;
		};

		led_power: power {
			label = "amber:power";
			gpios = <&gpio 2 GPIO_ACTIVE_LOW>;
			default-state = "on";
		};

		wlan2g {
			label = "blue:wlan2g";
			gpios = <&gpio 14 GPIO_ACTIVE_LOW>;
			linux,default-trigger = "phy1tpt";
		};
	};
};

&eth0 {
	status = "okay";

	pll-data = <0x06000000 0x00000101 0x00001616>;

	phy-mode = "rgmii";
	phy-handle = <&phy0>;

	gmac-config {
		device = <&gmac>;
		rgmii-gmac0 = <1>;
	};
};

&mdio0 {
	status = "okay";

	phy0: ethernet-phy@0 {
		reg = <0>;
		phy-mode = "rgmii";

		qca,ar8327-initvals = <
			0x04 0x87a00000 /* PORT0 PAD Mode */
			0x0c 0x01000000 /* PORT6 PAD Mode */
			0x10 0x80000000 /* PWS_REG_VALUE */
			0x7c 0x000000fe /* PORT0_STATUS */
			0x94 0x000000fe /* PORT6_STATUS */
		>;
	};
};

&pcie {
	status = "okay";

	wifi@0,0 {
		compatible = "qcom,ath10k";
		reg = <0x0000 0 0 0 0>;
	};
};

&ref {
	clock-frequency = <25000000>;
};

&spi {
	status = "okay";

	flash@0 {
		compatible = "jedec,spi-nor";
		reg = <0>;
		spi-max-frequency = <25000000>;

		partitions {
			compatible = "fixed-partitions";
			#address-cells = <1>;
			#size-cells = <1>;

			partition@0 {
				label = "u-boot";
				reg = <0x000000 0x030000>;
				read-only;
			};

			uenv: partition@30000 {
				label = "u-boot-env";
				reg = <0x030000 0x010000>;
				read-only;
			};

			partition@40000 {
				compatible = "denx,uimage";
				label = "firmware";
				reg = <0x040000 0x750000>;
			};

			partition@790000 {
				label = "backup";
				reg = <0x790000 0x010000>;
				read-only;
			};

			partition@7a0000 {
				label = "storage";
				reg = <0x7a0000 0x050000>;
				read-only;
			};

			art: partition@7f0000 {
				label = "art";
				reg = <0x7f0000 0x010000>;
				read-only;
			};
		};
	};
};

&usb {
	status = "okay";
};

&usb_phy {
	status = "okay";
};

&wmac {
	status = "okay";

	qca,no-eeprom;
};
