From 5aeffc428adfd3a97014056e36fd5496119da743 Mon Sep 17 00:00:00 2001
From: Dave Stevenson <dave.stevenson@raspberrypi.com>
Date: Tue, 3 Aug 2021 11:25:59 +0100
Subject: [PATCH] media: i2c: imx290: Add fwnode properties controls

Add call to v4l2_ctrl_new_fwnode_properties to read and
create the fwnode based controls.

Signed-off-by: Dave Stevenson <dave.stevenson@raspberrypi.com>
---
 drivers/media/i2c/imx290.c | 12 +++++++++++-
 1 file changed, 11 insertions(+), 1 deletion(-)

--- a/drivers/media/i2c/imx290.c
+++ b/drivers/media/i2c/imx290.c
@@ -1242,6 +1242,7 @@ static const struct of_device_id imx290_
 
 static int imx290_probe(struct i2c_client *client)
 {
+	struct v4l2_fwnode_device_properties props;
 	struct device *dev = &client->dev;
 	struct fwnode_handle *endpoint;
 	/* Only CSI2 is supported for now: */
@@ -1363,7 +1364,7 @@ static int imx290_probe(struct i2c_clien
 	 */
 	imx290_entity_init_cfg(&imx290->sd, NULL);
 
-	v4l2_ctrl_handler_init(&imx290->ctrls, 9);
+	v4l2_ctrl_handler_init(&imx290->ctrls, 11);
 
 	v4l2_ctrl_new_std(&imx290->ctrls, &imx290_ctrl_ops,
 			  V4L2_CID_ANALOGUE_GAIN, 0, 100, 1, 0);
@@ -1411,6 +1412,15 @@ static int imx290_probe(struct i2c_clien
 				     ARRAY_SIZE(imx290_test_pattern_menu) - 1,
 				     0, 0, imx290_test_pattern_menu);
 
+	ret = v4l2_fwnode_device_parse(&client->dev, &props);
+	if (ret)
+		goto free_ctrl;
+
+	ret = v4l2_ctrl_new_fwnode_properties(&imx290->ctrls, &imx290_ctrl_ops,
+					      &props);
+	if (ret)
+		goto free_ctrl;
+
 	imx290->sd.ctrl_handler = &imx290->ctrls;
 
 	if (imx290->ctrls.error) {
