#include "bcm6318.dtsi"

#include <dt-bindings/input/input.h>

/ {
	model = "Sagem F@st 2704N";
	compatible = "sagem,fast-2704n", "brcm,bcm6318";

	aliases {
		led-boot = &led_power_red;
		led-failsafe = &led_power_red;
		led-running = &led_power_red;
		led-upgrade = &led_power_red;
	};

	chosen {
		bootargs = "rootfstype=squashfs,jffs2 noinitrd console=ttyS0,115200";
		stdout-path = "serial0:115200n8";
	};

	keys {
		compatible = "gpio-keys-polled";
		#address-cells = <1>;
		#size-cells = <0>;
		poll-interval = <20>;

		wlan {
			label = "wlan";
			gpios = <&pinctrl 1 0>;
			linux,code = <KEY_WLAN>;
			debounce-interval = <60>;
		};

		wps {
			label = "wps";
			gpios = <&pinctrl 33 1>;
			linux,code = <KEY_WPS_BUTTON>;
			debounce-interval = <60>;
		};

		reset {
			label = "reset";
			gpios = <&pinctrl 34 1>;
			linux,code = <KEY_RESTART>;
			debounce-interval = <60>;
		};
	};

	leds {
		compatible = "gpio-leds";

		wps_green {
			label = "green:wps";
			gpios = <&pinctrl 2 1>;
		};
		lan1_green {
			label = "green:lan1";
			gpios = <&pinctrl 4 1>;
		};
		lan2_green {
			label = "green:lan2";
			gpios = <&pinctrl 5 1>;
		};
		lan3_green {
			label = "green:lan3";
			gpios = <&pinctrl 6 1>;
		};
		lan4_green {
			label = "green:lan4";
			gpios = <&pinctrl 7 1>;
		};
		inet_green {
			label = "green:inet";
			gpios = <&pinctrl 8 1>;
		};
		inet_red {
			label = "red:inet";
			gpios = <&pinctrl 9 1>;
		};
		dsl_green {
			label = "green:dsl";
			gpios = <&pinctrl 10 1>;
		};
		led_power_red: power_red {
			label = "red:power";
			gpios = <&pinctrl 11 1>;
		};
		power_green {
			label = "green:power";
			gpios = <&pinctrl 47 1>;
			default-state = "on";
		};
		usb_green {
			label = "green:usb";
			gpios = <&pinctrl 49 1>;
		};
	};
};

&hsspi {
	status = "okay";

	flash@0 {
		compatible = "jedec,spi-nor";
		spi-max-frequency = <62500000>;
		spi-tx-bus-width = <2>;
		spi-rx-bus-width = <2>;
		reg = <0>;

		#address-cells = <1>;
		#size-cells = <1>;

		partitions {
			compatible = "fixed-partitions";
			#address-cells = <1>;
			#size-cells = <1>;

			cfe@0 {
				reg = <0x000000 0x010000>;
				label = "cfe";
				read-only;
			};

			linux@10000 {
				reg = <0x010000 0x7e0000>;
				label = "linux";
				compatible = "brcm,bcm963xx-imagetag";
			};

			nvram@7f0000 {
				reg = <0x7f0000 0x010000>;
				label = "nvram";
			};
		};
	};
};

&uart0 {
	status = "okay";
};
