#include "danube.dtsi"

#include <dt-bindings/input/input.h>

/ {
	compatible = "arcadyan,arv4510pw", "lantiq,xway", "lantiq,danube";
	model = "Wippies, Elisa";

	chosen {
		bootargs = "console=ttyLTQ0,115200";
	};

	aliases {
		led-boot = &power;
		led-failsafe = &power2;
		led-running = &power;
		led-upgrade = &power;

		led-dsl = &adsl;
		led-internet = &internet;
		led-usb = &led_usb;
		led-usb2 = &led_usb2;
		led-wifi = &wifi;
	};

	memory@0 {
		device_type = "memory";
		reg = <0x0 0x2000000>;
	};

	keys {
		compatible = "gpio-keys-polled";
		poll-interval = <100>;

		wps {
			label = "wps";
			gpios = <&gpio 14 GPIO_ACTIVE_LOW>;
			linux,code = <KEY_WPS_BUTTON>;
		};
		reset {
			label = "reset";
			gpios = <&gpio 3 GPIO_ACTIVE_LOW>;
			linux,code = <KEY_RESTART>;
		};
	};

	leds {
		compatible = "gpio-leds";
		power: power {
			label = "power";
			gpios = <&gpios 21 GPIO_ACTIVE_HIGH>;
			default-state = "keep";
		};
		power2: power2 {
			label = "power2";
			gpios = <&gpios 20 GPIO_ACTIVE_HIGH>;
		};
		lan1 {
			label = "lan1";
			gpios = <&gpios 19 GPIO_ACTIVE_HIGH>;
		};
		lan2 {
			label = "lan2";
			gpios = <&gpios 18 GPIO_ACTIVE_HIGH>;
		};
		lan3 {
			label = "lan3";
			gpios = <&gpios 17 GPIO_ACTIVE_HIGH>;
		};
		lan4 {
			label = "lan4";
			gpios = <&gpios 16 GPIO_ACTIVE_HIGH>;
		};
		wifi: wifi {
			label = "wifi";
			gpios = <&gpios 15 GPIO_ACTIVE_HIGH>;
		};
		adsl: adsl {
			label = "adsl";
			gpios = <&gpios 14 GPIO_ACTIVE_HIGH>;
		};
		internet: internet {
			label = "internet";
			gpios = <&gpios 13 GPIO_ACTIVE_HIGH>;
		};
		internet2 {
			label = "internet2";
			gpios = <&gpios 12 GPIO_ACTIVE_HIGH>;
		};
		voip {
			label = "voip";
			gpios = <&gpios 11 GPIO_ACTIVE_HIGH>;
		};
		phone {
			label = "phone";
			gpios = <&gpios 10 GPIO_ACTIVE_HIGH>;
		};
		phone2 {
			label = "phone2";
			gpios = <&gpios 9 GPIO_ACTIVE_HIGH>;
		};
		led_usb: usb {
			label = "usb";
			gpios = <&gpios 8 GPIO_ACTIVE_HIGH>;
		};
		led_usb2: usb2 {
			label = "usb2";
			gpios = <&gpios 7 GPIO_ACTIVE_HIGH>;
		};
		usb3 {
			label = "usb3";
			gpios = <&gpios 6 GPIO_ACTIVE_HIGH>;
		};
		unlabeled {
			label = "unlabeled";
			gpios = <&gpios 5 GPIO_ACTIVE_HIGH>;
		};
	};
};

&gpio {
	pinctrl-names = "default";
	pinctrl-0 = <&state_default>;

	state_default: pinmux {
		ebu {
			lantiq,groups = "ebu a23";
			lantiq,function = "ebu";
			lantiq,open-drain = <0>;
			lantiq,output = <1>;
		};
		exin {
			lantiq,groups = "exin1", "exin2";
			lantiq,function = "exin";
			lantiq,output = <0>;
		};
		pci_rst {
			lantiq,pins = "io21";
			lantiq,open-drain = <0>;
			lantiq,output = <1>;
		};
		buttons {
			lantiq,pins = "io3", "io14";
			lantiq,pull = <2>;
			lantiq,output = <0>;
		};
	};
};

&gpios {
	status = "okay";
	lantiq,groups = <0x7>;
};

&gsw {
	phy-mode = "rmii";
};

&localbus {
	flash@0 {
		compatible = "lantiq,nor";
		bank-width = <2>;
		reg = <0 0x0 0x1000000>;

		lantiq,noxip;

		partitions {
			compatible = "fixed-partitions";
			#address-cells = <1>;
			#size-cells = <1>;

			partition@0 {
				label = "uboot";
				reg = <0x00000 0x40000>;
				read-only;
			};

			partition@40000 {
				label = "u-boot-env";
				reg = <0x40000 0x20000>;
				read-only;
			};

			partition@60000 {
				label = "firmware";
				reg = <0x60000 0xfa0000>;
			};
		};
	};
};

&pci0 {
	status = "okay";

	pinctrl-0 = <&pci_gnt1_pins>, <&pci_gnt2_pins>,
		    <&pci_req1_pins>, <&pci_req2_pins>;
	pinctrl-names = "default";

	lantiq,external-clock;
	interrupt-map = <
		0x6000 0 0 1 &icu0 135
		0x7800 0 0 1 &icu0 66
		0x7800 0 0 2 &icu0 66
		0x7800 0 0 3 &icu0 66
	>;
	gpio-reset = <&gpio 21 GPIO_ACTIVE_HIGH>;
	req-mask = <0x7>;
};

&vmmc {
	status = "okay";
};
