--- a/arch/mips/include/asm/octeon/cvmx-bootinfo.h
+++ b/arch/mips/include/asm/octeon/cvmx-bootinfo.h
@@ -297,7 +297,7 @@ enum cvmx_board_types_enum {
 	CVMX_BOARD_TYPE_UBNT_E100 = 20002,
 	CVMX_BOARD_TYPE_UBNT_E200 = 20003,
 	CVMX_BOARD_TYPE_UBNT_E220 = 20005,
-	CVMX_BOARD_TYPE_CUST_DSR1000N = 20006,
+	CVMX_BOARD_TYPE_ITUS_SHIELD = 20006,
 	CVMX_BOARD_TYPE_KONTRON_S1901 = 21901,
 	CVMX_BOARD_TYPE_CUST_PRIVATE_MAX = 30000,
 
@@ -400,7 +400,7 @@ static inline const char *cvmx_board_typ
 		ENUM_BRD_TYPE_CASE(CVMX_BOARD_TYPE_UBNT_E100)
 		ENUM_BRD_TYPE_CASE(CVMX_BOARD_TYPE_UBNT_E200)
 		ENUM_BRD_TYPE_CASE(CVMX_BOARD_TYPE_UBNT_E220)
-		ENUM_BRD_TYPE_CASE(CVMX_BOARD_TYPE_CUST_DSR1000N)
+		ENUM_BRD_TYPE_CASE(CVMX_BOARD_TYPE_ITUS_SHIELD)
 		ENUM_BRD_TYPE_CASE(CVMX_BOARD_TYPE_KONTRON_S1901)
 		ENUM_BRD_TYPE_CASE(CVMX_BOARD_TYPE_CUST_PRIVATE_MAX)
 	}
--- a/arch/mips/cavium-octeon/octeon-platform.c
+++ b/arch/mips/cavium-octeon/octeon-platform.c
@@ -771,7 +771,7 @@ int __init octeon_prune_device_tree(void
 	if (fdt_check_header(initial_boot_params))
 		panic("Corrupt Device Tree.");
 
-	WARN(octeon_bootinfo->board_type == CVMX_BOARD_TYPE_CUST_DSR1000N,
+	WARN(octeon_bootinfo->board_type == CVMX_BOARD_TYPE_ITUS_SHIELD,
 	     "Built-in DTB booting is deprecated on %s. Please switch to use appended DTB.",
 	     cvmx_board_type_to_string(octeon_bootinfo->board_type));
 
--- a/arch/mips/pci/pci-octeon.c
+++ b/arch/mips/pci/pci-octeon.c
@@ -211,8 +211,6 @@ const char *octeon_get_pci_interrupts(vo
 		return "AAABAAAAAAAAAAAAAAAAAAAAAAAAAAAA";
 	case CVMX_BOARD_TYPE_BBGW_REF:
 		return "AABCD";
-	case CVMX_BOARD_TYPE_CUST_DSR1000N:
-		return "CCCCCCCCCCCCCCCCCCCCCCCCCCCCCCCC";
 	case CVMX_BOARD_TYPE_THUNDER:
 	case CVMX_BOARD_TYPE_EBH3000:
 	default:
