#include "vr9.dtsi"

#include <dt-bindings/input/input.h>
#include <dt-bindings/mips/lantiq_rcu_gphy.h>

/ {
	compatible = "alphanetworks,asl56026", "lantiq,xway", "lantiq,vr9";
	model = "BT OpenReach VDSL Modem";

	chosen {
		bootargs = "console=ttyLTQ0,115200";
	};

	aliases {
		led-boot = &power_green;
		led-failsafe = &power_red;
		led-running = &power_green;
		led-upgrade = &power_green;

		led-dsl = &dsl;
	};

	memory@0 {
		device_type = "memory";
		reg = <0x0 0x2000000>;
	};

	keys {
		compatible = "gpio-keys-polled";
		poll-interval = <100>;

		reset {
			label = "reset";
			gpios = <&gpio 40 GPIO_ACTIVE_LOW>;
			linux,code = <KEY_RESTART>;
		};
	};

	leds {
		compatible = "gpio-leds";

		dsl: dsl {
			label = "green:dsl";
			gpios = <&gpio 6 GPIO_ACTIVE_LOW>;
		};

		/* power-* is a bicolour led */
		power_green: power_green {
			label = "green:power";
			gpios = <&gpio 17 GPIO_ACTIVE_HIGH>;
			default-state = "keep";
		};

		power_red: power_red {
			label = "red:power";
			gpios = <&gpio 18 GPIO_ACTIVE_HIGH>;
		};
	};

	gpio_export {
		compatible = "gpio-export";
		#size-cells = <0>;

		power_led_blink {
			gpio-export,name = "power_led_blink";
			gpio-export,output = <0>;
			gpios = <&gpio 16 GPIO_ACTIVE_LOW>;
		};
	};
};

&gphy0 {
	lantiq,gphy-mode = <GPHY_MODE_FE>;
};

&gphy1 {
	lantiq,gphy-mode = <GPHY_MODE_FE>;
};

&gswip_mdio {
	phy11: ethernet-phy@11 {
		reg = <0x11>;
	};

	phy14: ethernet-phy@14 {
		reg = <0x14>;
	};
};

&gswip_ports {
	port@2 {
		reg = <2>;
		label = "lan1";
		phy-mode = "internal";
		phy-handle = <&phy11>;
	};

	port@3 {
		reg = <3>;
		label = "lan2";
		phy-mode = "internal";
		phy-handle = <&phy14>;
	};
};

&localbus {
	flash@0 {
		compatible = "lantiq,nor";
		bank-width = <2>;
		reg = <0 0x0 0x0800000>;

		partitions {
			compatible = "fixed-partitions";
			#address-cells = <1>;
			#size-cells = <1>;

			partition@0 {
				label = "uboot";
				reg = <0x0 0x30000>;
			};

			partition@30000 {
				label = "u-boot-env";
				reg = <0x30000 0x10000>;
			};

			partition@40000 {
				label = "firmware";
				reg = <0x40000 0x750000>;
			};

			partition@790000 {
				label = "ddrconfig";
				reg = <0x790000 0x70000>;
				read-only;
			};
		};
	};
};
