// SPDX-License-Identifier: GPL-2.0-or-later OR MIT

#include "qca955x_senao_loader.dtsi"

#include <dt-bindings/gpio/gpio.h>
#include <dt-bindings/input/input.h>

/ {
	compatible = "engenius,eap1200h", "qca,qca9557";
	model = "EnGenius EAP1200H";

	aliases {
		label-mac-device = &eth0;
		led-boot = &led_power;
		led-failsafe = &led_power;
		led-running = &led_power;
		led-upgrade = &led_power;
	};

	keys {
		compatible = "gpio-keys";

		reset {
			label = "reset";
			gpios = <&gpio 17 GPIO_ACTIVE_LOW>;
			debounce-interval = <60>;
			linux,code = <KEY_RESTART>;
		};
	};

	leds {
		compatible = "gpio-leds";

		led_power: power {
			label = "amber:power";
			gpios = <&gpio 22 GPIO_ACTIVE_LOW>;
			default-state = "on";
		};

		wifi2g {
			label = "blue:wifi2g";
			gpios = <&gpio 13 GPIO_ACTIVE_LOW>;
			linux,default-trigger = "phy1tpt";
		};

		wifi5g {
			label = "green:wifi5g";
			gpios = <&gpio 23 GPIO_ACTIVE_LOW>;
			linux,default-trigger = "phy0tpt";
		};

		wps {
			label = "blue:wps";
			gpios = <&gpio 19 GPIO_ACTIVE_LOW>;
		};
	};
};

&partitions {
	art: partition@ff0000 {
		label = "art";
		reg = <0xff0000 0x010000>;
		read-only;
	};
};

&mdio0 {
	status = "okay";

	phy5: ethernet-phy@5 {
		reg = <5>;
		eee-broken-100tx;
		eee-broken-1000t;
	};
};

&eth0 {
	status = "okay";

	nvmem-cells = <&macaddr_art_0>;
	nvmem-cell-names = "mac-address";

	phy-handle = <&phy5>;
	phy-mode = "rgmii-id";

	pll-data = <0x82000000 0x80000101 0x80001313>;
};

&wmac {
	status = "okay";

	mtd-cal-data = <&art 0x1000>;
	nvmem-cells = <&macaddr_art_0>;
	nvmem-cell-names = "mac-address";
	mac-address-increment = <1>;
};

&art {
	compatible = "nvmem-cells";
	#address-cells = <1>;
	#size-cells = <1>;

	macaddr_art_0: macaddr@0 {
		reg = <0x0 0x6>;
	};
};
