From 33ef960aed15f9a98a2c51d8d794cd72418e0be4 Mon Sep 17 00:00:00 2001
From: Florian Fainelli <florian@openwrt.org>
Date: Mon, 28 Jan 2013 20:06:25 +0100
Subject: [PATCH 07/11] MIPS: BCM63XX: register OHCI controller if board
 enables it

BCM63XX-based boards can control the registration of the OHCI controller
by setting their has_ohci0 flag to 1. Handle this in the generic
code dealing with board registration and call the actual helper to
register the OHCI controller.

Signed-off-by: Florian Fainelli <florian@openwrt.org>
---
 arch/mips/bcm63xx/boards/board_bcm963xx.c |    4 ++++
 1 file changed, 4 insertions(+)

--- a/arch/mips/bcm63xx/boards/board_bcm963xx.c
+++ b/arch/mips/bcm63xx/boards/board_bcm963xx.c
@@ -27,6 +27,7 @@
 #include <bcm63xx_dev_hsspi.h>
 #include <bcm63xx_dev_pcmcia.h>
 #include <bcm63xx_dev_spi.h>
+#include <bcm63xx_dev_usb_ohci.h>
 #include <bcm63xx_dev_usb_usbd.h>
 #include <board_bcm963xx.h>
 
@@ -892,6 +893,9 @@ int __init board_register_devices(void)
 	if (board.has_usbd)
 		bcm63xx_usbd_register(&board.usbd);
 
+	if (board.has_ohci0)
+		bcm63xx_ohci_register();
+
 	/* Generate MAC address for WLAN and register our SPROM,
 	 * do this after registering enet devices
 	 */
