From 0e89c0d8e8edece7f8e4607841ca6651885d23b1 Mon Sep 17 00:00:00 2001
From: =?UTF-8?q?Rafa=C5=82=20Mi=C5=82ecki?= <rafal@milecki.pl>
Date: Thu, 19 Aug 2021 08:57:00 +0200
Subject: [PATCH] ARM: dts: BCM5301X: Fix nodes names
MIME-Version: 1.0
Content-Type: text/plain; charset=UTF-8
Content-Transfer-Encoding: 8bit

This fixes following errors for all BCM5301X dts files:
chipcommonA@18000000: $nodename:0: 'chipcommonA@18000000' does not match '^([a-z][a-z0-9\\-]+-bus|bus|soc|axi|ahb|apb)(@[0-9a-f]+)?$'
mpcore@19000000: $nodename:0: 'mpcore@19000000' does not match '^([a-z][a-z0-9\\-]+-bus|bus|soc|axi|ahb|apb)(@[0-9a-f]+)?$'
mdio-bus-mux@18003000: $nodename:0: 'mdio-bus-mux@18003000' does not match '^mdio-mux[\\-@]?'
dmu@1800c000: $nodename:0: 'dmu@1800c000' does not match '^([a-z][a-z0-9\\-]+-bus|bus|soc|axi|ahb|apb)(@[0-9a-f]+)?$'

Signed-off-by: Rafał Miłecki <rafal@milecki.pl>
Signed-off-by: Florian Fainelli <f.fainelli@gmail.com>
---
 arch/arm/boot/dts/bcm47094-linksys-panamera.dts | 2 +-
 arch/arm/boot/dts/bcm5301x.dtsi                 | 8 ++++----
 2 files changed, 5 insertions(+), 5 deletions(-)

--- a/arch/arm/boot/dts/bcm47094-linksys-panamera.dts
+++ b/arch/arm/boot/dts/bcm47094-linksys-panamera.dts
@@ -129,7 +129,7 @@
 		};
 	};
 
-	mdio-bus-mux@18003000 {
+	mdio-mux@18003000 {
 
 		/* BIT(9) = 1 => external mdio */
 		mdio@200 {
--- a/arch/arm/boot/dts/bcm5301x.dtsi
+++ b/arch/arm/boot/dts/bcm5301x.dtsi
@@ -19,7 +19,7 @@
 	#size-cells = <1>;
 	interrupt-parent = <&gic>;
 
-	chipcommonA@18000000 {
+	chipcommon-a-bus@18000000 {
 		compatible = "simple-bus";
 		ranges = <0x00000000 0x18000000 0x00001000>;
 		#address-cells = <1>;
@@ -44,7 +44,7 @@
 		};
 	};
 
-	mpcore@19000000 {
+	mpcore-bus@19000000 {
 		compatible = "simple-bus";
 		ranges = <0x00000000 0x19000000 0x00023000>;
 		#address-cells = <1>;
@@ -369,7 +369,7 @@
 		#address-cells = <1>;
 	};
 
-	mdio-bus-mux@18003000 {
+	mdio-mux@18003000 {
 		compatible = "mdio-mux-mmioreg";
 		mdio-parent-bus = <&mdio>;
 		#address-cells = <1>;
@@ -415,7 +415,7 @@
 		status = "disabled";
 	};
 
-	dmu@1800c000 {
+	dmu-bus@1800c000 {
 		compatible = "simple-bus";
 		ranges = <0 0x1800c000 0x1000>;
 		#address-cells = <1>;
