From bdc34f2e9bd66e717888a1867e540a6b4f85b55d Mon Sep 17 00:00:00 2001
From: Dave Stevenson <dave.stevenson@raspberrypi.com>
Date: Wed, 1 Jul 2020 10:57:57 +0100
Subject: [PATCH] media: bcm2835-unicam: Add support for unpacked 14bit
 Bayer formats

Now that the 14bit non-packed Bayer formats are defined, add them
into the supported formats lookup table.

Signed-off-by: Dave Stevenson <dave.stevenson@raspberrypi.com>
---
 drivers/media/platform/bcm2835/bcm2835-unicam.c | 4 ++++
 1 file changed, 4 insertions(+)

--- a/drivers/media/platform/bcm2835/bcm2835-unicam.c
+++ b/drivers/media/platform/bcm2835/bcm2835-unicam.c
@@ -299,21 +299,25 @@ static const struct unicam_fmt formats[]
 		.csi_dt		= 0x2c,
 	}, {
 		.fourcc		= V4L2_PIX_FMT_SBGGR14P,
+		.repacked_fourcc = V4L2_PIX_FMT_SBGGR14,
 		.code		= MEDIA_BUS_FMT_SBGGR14_1X14,
 		.depth		= 14,
 		.csi_dt		= 0x2d,
 	}, {
 		.fourcc		= V4L2_PIX_FMT_SGBRG14P,
+		.repacked_fourcc = V4L2_PIX_FMT_SGBRG14,
 		.code		= MEDIA_BUS_FMT_SGBRG14_1X14,
 		.depth		= 14,
 		.csi_dt		= 0x2d,
 	}, {
 		.fourcc		= V4L2_PIX_FMT_SGRBG14P,
+		.repacked_fourcc = V4L2_PIX_FMT_SGRBG14,
 		.code		= MEDIA_BUS_FMT_SGRBG14_1X14,
 		.depth		= 14,
 		.csi_dt		= 0x2d,
 	}, {
 		.fourcc		= V4L2_PIX_FMT_SRGGB14P,
+		.repacked_fourcc = V4L2_PIX_FMT_SRGGB14,
 		.code		= MEDIA_BUS_FMT_SRGGB14_1X14,
 		.depth		= 14,
 		.csi_dt		= 0x2d,
