// SPDX-License-Identifier: GPL-2.0-or-later OR MIT

#include "qca9556_avm_fritz-repeater.dtsi"

#include <dt-bindings/gpio/gpio.h>

/ {
	compatible = "avm,fritz1750e", "qca,qca9556";
	model = "AVM FRITZ!WLAN Repeater 1750E";

	aliases {
		led-boot = &led_power;
		led-failsafe = &led_power;
		led-running = &led_power;
		led-upgrade = &led_power;
	};

	led_spi {
		compatible = "spi-gpio";
		#address-cells = <1>;
		#size-cells = <0>;

		sck-gpios = <&gpio 14 GPIO_ACTIVE_HIGH>;
		mosi-gpios = <&gpio 15 GPIO_ACTIVE_HIGH>;
		num-chipselects = <0>;

		spi_gpio: led_gpio@0 {
			compatible = "fairchild,74hc595";
			reg = <0>;
			gpio-controller;
			#gpio-cells = <2>;
			registers-number = <1>;
			spi-max-frequency = <10000000>;

			gpio_latch_bit {
				gpio-hog;
				gpios = <7 GPIO_ACTIVE_HIGH>;
				output-high;
				line-name = "gpio-latch-bit";
			};
		};
	};

	leds {
		compatible = "gpio-leds";

		led_power: power {
			label = "green:power";
			gpios = <&spi_gpio 6 GPIO_ACTIVE_HIGH>;
		};

		wlan {
			label = "green:wlan";
			gpios = <&spi_gpio 5 GPIO_ACTIVE_HIGH>;
			linux,default-trigger = "phy1tpt";
		};

		lan {
			label = "green:lan";
			gpios = <&gpio 13 GPIO_ACTIVE_HIGH>;
		};

		rssi0 {
			label = "green:rssi0";
			gpios = <&spi_gpio 0 GPIO_ACTIVE_HIGH>;
		};

		rssi1 {
			label = "green:rssi1";
			gpios = <&spi_gpio 1 GPIO_ACTIVE_HIGH>;
		};

		rssi2 {
			label = "green:rssi2";
			gpios = <&spi_gpio 2 GPIO_ACTIVE_HIGH>;
		};

		rssi3 {
			label = "green:rssi3";
			gpios = <&spi_gpio 3 GPIO_ACTIVE_HIGH>;
		};

		rssi4 {
			label = "green:rssi4";
			gpios = <&spi_gpio 4 GPIO_ACTIVE_HIGH>;
		};
	};
};

&pcie0 {
	status = "okay";
};

&phy0 {
	reset-gpios = <&gpio 11 GPIO_ACTIVE_LOW>;
};

&gpio {
	reset-pcie-ep {
		gpio-hog;
		gpios = <17 GPIO_ACTIVE_HIGH>;
		output-high;
		line-name = "PCIE EP reset";
	};

	reset-pcie {
		gpio-hog;
		gpios = <18 GPIO_ACTIVE_HIGH>;
		output-high;
		line-name = "PCIE Bus reset";
	};
};
