--- a/drivers/mtd/spi/spi-nor-ids.c
+++ b/drivers/mtd/spi/spi-nor-ids.c
@@ -353,6 +353,8 @@ const struct flash_info spi_nor_ids[] =
 			SPI_NOR_HAS_LOCK | SPI_NOR_HAS_TB)
 	},
 	{ INFO("w25q256", 0xef4019, 0, 64 * 1024, 512, SECT_4K | SPI_NOR_DUAL_READ | SPI_NOR_QUAD_READ) },
+	{ INFO("w25q512jv", 0xef4020, 0, 64 * 1024, 1024, SECT_4K | SPI_NOR_QUAD_READ | SPI_NOR_DUAL_READ |
+			SPI_NOR_HAS_TB | SPI_NOR_HAS_LOCK) },
 	{ INFO("w25m512jw", 0xef6119, 0, 64 * 1024, 1024, SECT_4K | SPI_NOR_DUAL_READ | SPI_NOR_QUAD_READ) },
 	{ INFO("w25m512jv", 0xef7119, 0, 64 * 1024, 1024, SECT_4K | SPI_NOR_DUAL_READ | SPI_NOR_QUAD_READ) },
 #endif
