// SPDX-License-Identifier: GPL-2.0-or-later OR MIT

#include "mt7621.dtsi"

#include <dt-bindings/gpio/gpio.h>
#include <dt-bindings/input/input.h>

/ {
	compatible = "wavlink,wl-wn531a6", "mediatek,mt7621-soc";
	model = "Wavlink WL-WN531A6";

	aliases {
		led-boot = &led_status_red;
		led-failsafe = &led_status_red;
		led-running = &led_status_blue;
		led-upgrade = &led_status_red;
	};

	keys {
		compatible = "gpio-keys";

		reset {
			label = "Reset Button";
			gpios = <&gpio 18 GPIO_ACTIVE_LOW>;
			linux,code = <KEY_RESTART>;
		};

		touch { /* RH6015C touch sensor -> GPIO 14 */
			label = "Touch Button";
			gpios = <&gpio 14 GPIO_ACTIVE_LOW>;
			linux,code = <BTN_0>;
		};

		turbo {
			label = "Turbo Button";
			gpios = <&gpio 25 GPIO_ACTIVE_LOW>;
			linux,code = <BTN_1>;
		};

		wps {
			label = "WPS Button";
			gpios = <&gpio 24 GPIO_ACTIVE_LOW>;
			linux,code = <KEY_WPS_BUTTON>;
		};
	};

	leds {
		compatible = "gpio-leds";

		led_status_blue: status_blue {
			label = "blue:power";
			gpios = <&gpio 16 GPIO_ACTIVE_HIGH>;
		};

		led_status_red: status_red {
			label = "red:power";
			gpios = <&gpio 17 GPIO_ACTIVE_HIGH>;
		};

		wifi2g {
			label = "blue:wifi2g";
			gpios = <&gpio 23 GPIO_ACTIVE_LOW>;
			linux,default-trigger = "phy0tpt";
		};
	};
};

&i2c {
	status = "okay";
};

&spi0 {
	status = "okay";

	flash@0 {
		compatible = "jedec,spi-nor";
		reg = <0>;
		spi-max-frequency = <40000000>;

		partitions {
			compatible = "fixed-partitions";
			#address-cells = <1>;
			#size-cells = <1>;

			partition@0 {
				label = "u-boot";
				reg = <0x0 0x30000>;
				read-only;
			};

			partition@30000 {
				label = "config";
				reg = <0x30000 0x10000>;
				read-only;
			};

			factory: partition@40000 {
				label = "factory";
				reg = <0x40000 0x10000>;
				read-only;
			};

			partition@50000 {
				compatible = "denx,uimage";
				label = "firmware";
				reg = <0x50000 0xeb0000>;
			};

			partition@f00000 {
				label = "vendor";
				reg = <0xf00000 0x100000>;
				read-only;
			};
		};
	};
};

&pcie {
	status = "okay";
};

&pcie0 {
	mt76@0,0 {
		compatible = "mediatek,mt76";
		reg = <0x0000 0 0 0 0>;
		mediatek,mtd-eeprom = <&factory 0x0>;
		ieee80211-freq-limit = <2400000 2500000>;
	};
};

&pcie1 {
	mt76@0,0 {
		compatible = "mediatek,mt76";
		reg = <0x0000 0 0 0 0>;
		mediatek,mtd-eeprom = <&factory 0x8000>;
		ieee80211-freq-limit = <5000000 6000000>;
	};
};

&gmac0 {
	nvmem-cells = <&macaddr_factory_e000>;
	nvmem-cell-names = "mac-address";
};

&switch0 {
	ports {
		port@0 {
			status = "okay";
			label = "lan1";
		};

		port@1 {
			status = "okay";
			label = "lan2";
		};

		port@2 {
			status = "okay";
			label = "lan3";
		};

		port@3 {
			status = "okay";
			label = "lan4";
		};

		port@4 {
			status = "okay";
			label = "wan";
			nvmem-cells = <&macaddr_factory_e006>;
			nvmem-cell-names = "mac-address";
		};
	};
};

&state_default {
	gpio {
		groups = "rgmii2", "jtag", "wdt";
		function = "gpio";
	};
};

&uartlite2 {
	status = "okay";
};

&factory {
	compatible = "nvmem-cells";
	#address-cells = <1>;
	#size-cells = <1>;

	macaddr_factory_e000: macaddr@e000 {
		reg = <0xe000 0x6>;
	};

	macaddr_factory_e006: macaddr@e006 {
		reg = <0xe006 0x6>;
	};
};
