From 069990e0b524a7acdcfef0505913ee20401fec5a Mon Sep 17 00:00:00 2001
From: Phil Elwell <phil@raspberrypi.org>
Date: Mon, 6 Jan 2020 14:05:42 +0000
Subject: [PATCH] pinctrl: bcm2835: Change init order for gpio hogs

pinctrl-bcm2835 is a combined pinctrl/gpio driver. Currently the gpio
side is registered first, but this breaks gpio hogs (which are
configured during gpiochip_add_data). Part of the hog initialisation
is a call to pinctrl_gpio_request, and since the pinctrl driver hasn't
yet been registered this results in an -EPROBE_DEFER from which it can
never recover.

Change the initialisation sequence to register the pinctrl driver
first.

See: https://www.raspberrypi.org/forums/viewtopic.php?f=107&t=260600

Signed-off-by: Phil Elwell <phil@raspberrypi.org>
---
 drivers/pinctrl/bcm/pinctrl-bcm2835.c | 29 +++++++++++++++------------
 1 file changed, 16 insertions(+), 13 deletions(-)

--- a/drivers/pinctrl/bcm/pinctrl-bcm2835.c
+++ b/drivers/pinctrl/bcm/pinctrl-bcm2835.c
@@ -1244,6 +1244,18 @@ static int bcm2835_pinctrl_probe(struct
 		raw_spin_lock_init(&pc->irq_lock[i]);
 	}
 
+	pc->pctl_desc = *pdata->pctl_desc;
+	pc->pctl_dev = devm_pinctrl_register(dev, &pc->pctl_desc, pc);
+	if (IS_ERR(pc->pctl_dev)) {
+		gpiochip_remove(&pc->gpio_chip);
+		return PTR_ERR(pc->pctl_dev);
+	}
+
+	pc->gpio_range = *pdata->gpio_range;
+	pc->gpio_range.base = pc->gpio_chip.base;
+	pc->gpio_range.gc = &pc->gpio_chip;
+	pinctrl_add_gpio_range(pc->pctl_dev, &pc->gpio_range);
+
 	girq = &pc->gpio_chip.irq;
 	girq->chip = &bcm2835_gpio_irq_chip;
 	girq->parent_handler = bcm2835_gpio_irq_handler;
@@ -1251,8 +1263,10 @@ static int bcm2835_pinctrl_probe(struct
 	girq->parents = devm_kcalloc(dev, BCM2835_NUM_IRQS,
 				     sizeof(*girq->parents),
 				     GFP_KERNEL);
-	if (!girq->parents)
+	if (!girq->parents) {
+		pinctrl_remove_gpio_range(pc->pctl_dev, &pc->gpio_range);
 		return -ENOMEM;
+	}
 
 	if (is_7211) {
 		pc->wake_irq = devm_kcalloc(dev, BCM2835_NUM_IRQS,
@@ -1303,21 +1317,10 @@ static int bcm2835_pinctrl_probe(struct
 	err = devm_gpiochip_add_data(dev, &pc->gpio_chip, pc);
 	if (err) {
 		dev_err(dev, "could not add GPIO chip\n");
+		pinctrl_remove_gpio_range(pc->pctl_dev, &pc->gpio_range);
 		return err;
 	}
 
-	pc->pctl_desc = *pdata->pctl_desc;
-	pc->pctl_dev = devm_pinctrl_register(dev, &pc->pctl_desc, pc);
-	if (IS_ERR(pc->pctl_dev)) {
-		gpiochip_remove(&pc->gpio_chip);
-		return PTR_ERR(pc->pctl_dev);
-	}
-
-	pc->gpio_range = *pdata->gpio_range;
-	pc->gpio_range.base = pc->gpio_chip.base;
-	pc->gpio_range.gc = &pc->gpio_chip;
-	pinctrl_add_gpio_range(pc->pctl_dev, &pc->gpio_range);
-
 	return 0;
 }
 
