From 0e28623a11f3916c1fe5b7e789c7ab8ca932a929 Mon Sep 17 00:00:00 2001
From: Robert Marko <robimarko@gmail.com>
Date: Wed, 22 Jan 2020 13:02:13 +0100
Subject: [PATCH] mmc: sdhci: sdhci-msm: use sdhci_set_clock instead of
 sdhci_msm_set_clock

When using sdhci_msm_set_clock clock setting will fail, so lets
use the generic sdhci_set_clock.

Signed-off-by: Robert Marko <robimarko@gmail.com>
---
 drivers/mmc/host/sdhci-msm.c | 2 +-
 1 file changed, 1 insertion(+), 1 deletion(-)

--- a/drivers/mmc/host/sdhci-msm.c
+++ b/drivers/mmc/host/sdhci-msm.c
@@ -1763,7 +1763,7 @@ MODULE_DEVICE_TABLE(of, sdhci_msm_dt_mat
 
 static const struct sdhci_ops sdhci_msm_ops = {
 	.reset = sdhci_reset,
-	.set_clock = sdhci_msm_set_clock,
+	.set_clock = sdhci_set_clock,
 	.get_min_clock = sdhci_msm_get_min_clock,
 	.get_max_clock = sdhci_msm_get_max_clock,
 	.set_bus_width = sdhci_set_bus_width,
