--- a/arch/mips/pci/ifxmips_pcie.c
+++ b/arch/mips/pci/ifxmips_pcie.c
@@ -16,8 +16,15 @@
 #include <asm/paccess.h>
 #include <linux/pci.h>
 #include <linux/pci_regs.h>
+#include <linux/phy/phy.h>
+#include <linux/regmap.h>
+#include <linux/reset.h>
+#include <linux/mfd/syscon.h>
 #include <linux/module.h>
 
+#include <linux/of_gpio.h>
+#include <linux/of_platform.h>
+
 #include "ifxmips_pcie.h"
 #include "ifxmips_pcie_reg.h"
 
@@ -40,6 +47,10 @@
 static DEFINE_SPINLOCK(ifx_pcie_lock);
 
 u32 g_pcie_debug_flag = PCIE_MSG_ANY & (~PCIE_MSG_CFG);
+static int pcie_reset_gpio;
+static struct phy *ltq_pcie_phy;
+static struct reset_control *ltq_pcie_reset;
+static struct regmap *ltq_rcu_regmap;
 
 static ifx_pcie_irq_t pcie_irqs[IFX_PCIE_CORE_NR] = {
     {
@@ -82,6 +93,22 @@ void ifx_pcie_debug(const char *fmt, ...
 	printk("%s", buf);
 }
 
+static inline void pcie_ep_gpio_rst_init(int pcie_port)
+{
+	gpio_direction_output(pcie_reset_gpio, 1);
+	gpio_set_value(pcie_reset_gpio, 1);
+}
+
+static inline void pcie_device_rst_assert(int pcie_port)
+{
+	gpio_set_value(pcie_reset_gpio, 0);
+}
+
+static inline void pcie_device_rst_deassert(int pcie_port)
+{
+	mdelay(100);
+	gpio_direction_output(pcie_reset_gpio, 1);
+}
 
 static inline int pcie_ltssm_enable(int pcie_port)
 {
@@ -988,10 +1015,22 @@ int  ifx_pcie_bios_plat_dev_init(struct
 static int
 pcie_rc_initialize(int pcie_port)
 {
-	int i;
+	int i, ret;
 #define IFX_PCIE_PHY_LOOP_CNT  5
 
-	pcie_rcu_endian_setup(pcie_port);
+	regmap_update_bits(ltq_rcu_regmap, 0x4c, IFX_RCU_AHB_BE_PCIE_M,
+			   IFX_RCU_AHB_BE_PCIE_M);
+
+#ifdef CONFIG_IFX_PCIE_HW_SWAP
+	regmap_update_bits(ltq_rcu_regmap, 0x4c, IFX_RCU_AHB_BE_PCIE_S,
+			   IFX_RCU_AHB_BE_PCIE_S);
+#else
+	regmap_update_bits(ltq_rcu_regmap, 0x4c, IFX_RCU_AHB_BE_PCIE_S,
+			   0x0);
+#endif
+
+	regmap_update_bits(ltq_rcu_regmap, 0x4c, IFX_RCU_AHB_BE_XBAR_M,
+			   0x0);
 
 	pcie_ep_gpio_rst_init(pcie_port);
 
@@ -1000,26 +1039,21 @@ pcie_rc_initialize(int pcie_port)
 	* reset PCIe PHY will solve this issue 
 	*/
 	for (i = 0; i < IFX_PCIE_PHY_LOOP_CNT; i++) {
-		/* Disable PCIe PHY Analog part for sanity check */
-		pcie_phy_pmu_disable(pcie_port);
-
-		pcie_phy_rst_assert(pcie_port);
-		pcie_phy_rst_deassert(pcie_port);
-
-		/* Make sure PHY PLL is stable */
-		udelay(20);
-
-		/* PCIe Core reset enabled, low active, sw programmed */
-		pcie_core_rst_assert(pcie_port);
+		ret = phy_init(ltq_pcie_phy);
+		if (ret)
+			continue;
 
 		/* Put PCIe EP in reset status */
 		pcie_device_rst_assert(pcie_port);
 
-		/* PCI PHY & Core reset disabled, high active, sw programmed */
-		pcie_core_rst_deassert(pcie_port);
+		udelay(1);
+		reset_control_deassert(ltq_pcie_reset);
 
-		/* Already in a quiet state, program PLL, enable PHY, check ready bit */
-		pcie_phy_clock_mode_setup(pcie_port);
+		ret = phy_power_on(ltq_pcie_phy);
+		if (ret) {
+			phy_exit(ltq_pcie_phy);
+			continue;
+		}
 
 		/* Enable PCIe PHY and Clock */
 		pcie_core_pmu_setup(pcie_port);
@@ -1035,6 +1069,10 @@ pcie_rc_initialize(int pcie_port)
 		/* Once link is up, break out */
 		if (pcie_app_loigc_setup(pcie_port) == 0)
 			break;
+
+		phy_power_off(ltq_pcie_phy);
+		reset_control_assert(ltq_pcie_reset);
+		phy_exit(ltq_pcie_phy);
 	}
 	if (i >= IFX_PCIE_PHY_LOOP_CNT) {
 		printk(KERN_ERR "%s link up failed!!!!!\n", __func__);
@@ -1045,17 +1083,67 @@ pcie_rc_initialize(int pcie_port)
 	return 0;
 }
 
-static int __init ifx_pcie_bios_init(void)
+static int ifx_pcie_bios_probe(struct platform_device *pdev)
 {
+    struct device_node *node = pdev->dev.of_node;
     void __iomem *io_map_base;
     int pcie_port;
     int startup_port;
+    struct device_node *np;
+    struct pci_bus *bus;
+
+    /*
+     * In case a PCI device is physical present, the Lantiq PCI driver need
+     * to be loaded prior to the Lantiq PCIe driver. Otherwise none of them
+     * will work.
+     *
+     * In case the lantiq PCI driver is enabled in the device tree, check if
+     * a PCI bus (hopefully the one of the Lantiq PCI driver one) is already
+     * registered.
+     *
+     * It will fail if there is another PCI controller, this controller is
+     * registered before the Lantiq PCIe driver is probe and the lantiq PCI
+     */
+    np = of_find_compatible_node(NULL, NULL, "lantiq,pci-xway");
+
+    if (of_device_is_available(np)) {
+        bus = pci_find_next_bus(bus);
+
+        if (!bus)
+	     return -EPROBE_DEFER;
+    }
 
     /* Enable AHB Master/ Slave */
     pcie_ahb_pmu_setup();
 
     startup_port = IFX_PCIE_PORT0;
-    
+
+    ltq_pcie_phy = devm_phy_get(&pdev->dev, "pcie");
+    if (IS_ERR(ltq_pcie_phy)) {
+        dev_err(&pdev->dev, "failed to get the PCIe PHY\n");
+        return PTR_ERR(ltq_pcie_phy);
+    }
+
+    ltq_pcie_reset = devm_reset_control_get_shared(&pdev->dev, NULL);
+    if (IS_ERR(ltq_pcie_reset)) {
+        dev_err(&pdev->dev, "failed to get the PCIe reset line\n");
+        return PTR_ERR(ltq_pcie_reset);
+    }
+
+    ltq_rcu_regmap = syscon_regmap_lookup_by_phandle(node, "lantiq,rcu");
+    if (IS_ERR(ltq_rcu_regmap))
+        return PTR_ERR(ltq_rcu_regmap);
+
+    pcie_reset_gpio = of_get_named_gpio(node, "gpio-reset", 0);
+    if (gpio_is_valid(pcie_reset_gpio)) {
+        int ret = devm_gpio_request(&pdev->dev, pcie_reset_gpio, "pcie-reset");
+        if (ret) {
+            dev_err(&pdev->dev, "failed to request gpio %d\n", pcie_reset_gpio);
+            return ret;
+        }
+        gpio_direction_output(pcie_reset_gpio, 1);
+    }
+
     for (pcie_port = startup_port; pcie_port < IFX_PCIE_CORE_NR; pcie_port++){
 	if (pcie_rc_initialize(pcie_port) == 0) {
 	    IFX_PCIE_PRINT(PCIE_MSG_INIT, "%s: ifx_pcie_cfg_base 0x%p\n", 
@@ -1067,6 +1155,7 @@ static int __init ifx_pcie_bios_init(voi
                 return -ENOMEM;
             }
             ifx_pcie_controller[pcie_port].pcic.io_map_base = (unsigned long)io_map_base;
+            pci_load_of_ranges(&ifx_pcie_controller[pcie_port].pcic, node);
 
             register_pci_controller(&ifx_pcie_controller[pcie_port].pcic);
             /* XXX, clear error status */
@@ -1083,6 +1172,30 @@ static int __init ifx_pcie_bios_init(voi
 
     return 0;
 }
+
+static const struct of_device_id ifxmips_pcie_match[] = {
+        { .compatible = "lantiq,pcie-xrx200" },
+        {},
+};
+MODULE_DEVICE_TABLE(of, ifxmips_pcie_match);
+
+static struct platform_driver ltq_pci_driver = {
+        .probe = ifx_pcie_bios_probe,
+        .driver = {
+                .name = "pcie-xrx200",
+                .owner = THIS_MODULE,
+                .of_match_table = ifxmips_pcie_match,
+        },
+};
+
+int __init ifx_pcie_bios_init(void)
+{
+        int ret = platform_driver_register(&ltq_pci_driver);
+        if (ret)
+                pr_info("pcie-xrx200: Error registering platform driver!");
+        return ret;
+}
+
 arch_initcall(ifx_pcie_bios_init);
 
 MODULE_LICENSE("GPL");
--- a/arch/mips/pci/ifxmips_pcie_vr9.h
+++ b/arch/mips/pci/ifxmips_pcie_vr9.h
@@ -22,8 +22,6 @@
 #include <linux/gpio.h>
 #include <lantiq_soc.h>
 
-#define IFX_PCIE_GPIO_RESET  494
-
 #define IFX_REG_R32    ltq_r32
 #define IFX_REG_W32    ltq_w32
 #define CONFIG_IFX_PCIE_HW_SWAP
@@ -53,21 +51,6 @@
 #define OUT			((volatile u32*)(IFX_GPIO + 0x0070))
 
 
-static inline void pcie_ep_gpio_rst_init(int pcie_port)
-{
-
-	gpio_request(IFX_PCIE_GPIO_RESET, "pcie-reset");
-	gpio_direction_output(IFX_PCIE_GPIO_RESET, 1);
-	gpio_set_value(IFX_PCIE_GPIO_RESET, 1);
-
-/*    ifx_gpio_pin_reserve(IFX_PCIE_GPIO_RESET, ifx_pcie_gpio_module_id);
-    ifx_gpio_output_set(IFX_PCIE_GPIO_RESET, ifx_pcie_gpio_module_id);
-    ifx_gpio_dir_out_set(IFX_PCIE_GPIO_RESET, ifx_pcie_gpio_module_id);
-    ifx_gpio_altsel0_clear(IFX_PCIE_GPIO_RESET, ifx_pcie_gpio_module_id);
-    ifx_gpio_altsel1_clear(IFX_PCIE_GPIO_RESET, ifx_pcie_gpio_module_id);
-    ifx_gpio_open_drain_set(IFX_PCIE_GPIO_RESET, ifx_pcie_gpio_module_id);*/
-}
-
 static inline void pcie_ahb_pmu_setup(void) 
 {
 	/* Enable AHB bus master/slave */
@@ -79,24 +62,6 @@ static inline void pcie_ahb_pmu_setup(vo
     //AHBS_PMU_SETUP(IFX_PMU_ENABLE);
 }
 
-static inline void pcie_rcu_endian_setup(int pcie_port)
-{
-    u32 reg;
-
-    reg = IFX_REG_R32(IFX_RCU_AHB_ENDIAN);
-#ifdef CONFIG_IFX_PCIE_HW_SWAP
-    reg |= IFX_RCU_AHB_BE_PCIE_M;
-    reg |= IFX_RCU_AHB_BE_PCIE_S;
-    reg &= ~IFX_RCU_AHB_BE_XBAR_M;
-#else 
-    reg |= IFX_RCU_AHB_BE_PCIE_M;
-    reg &= ~IFX_RCU_AHB_BE_PCIE_S;
-    reg &= ~IFX_RCU_AHB_BE_XBAR_M;
-#endif /* CONFIG_IFX_PCIE_HW_SWAP */
-    IFX_REG_W32(reg, IFX_RCU_AHB_ENDIAN);
-    IFX_PCIE_PRINT(PCIE_MSG_REG, "%s IFX_RCU_AHB_ENDIAN: 0x%08x\n", __func__, IFX_REG_R32(IFX_RCU_AHB_ENDIAN));
-}
-
 static inline void pcie_phy_pmu_enable(int pcie_port)
 {
 	struct clk *clk;
@@ -115,17 +80,6 @@ static inline void pcie_phy_pmu_disable(
 //    PCIE_PHY_PMU_SETUP(IFX_PMU_DISABLE);
 }
 
-static inline void pcie_pdi_big_endian(int pcie_port)
-{
-    u32 reg;
-
-    /* SRAM2PDI endianness control. */
-    reg = IFX_REG_R32(IFX_RCU_AHB_ENDIAN);
-    /* Config AHB->PCIe and PDI endianness */
-    reg |= IFX_RCU_AHB_BE_PCIE_PDI;
-    IFX_REG_W32(reg, IFX_RCU_AHB_ENDIAN);
-}
-
 static inline void pcie_pdi_pmu_enable(int pcie_port)
 {
     /* Enable PDI to access PCIe PHY register */
@@ -135,65 +89,6 @@ static inline void pcie_pdi_pmu_enable(i
     //PDI_PMU_SETUP(IFX_PMU_ENABLE);
 }
 
-static inline void pcie_core_rst_assert(int pcie_port)
-{
-    u32 reg;
-
-    reg = IFX_REG_R32(IFX_RCU_RST_REQ);
-
-    /* Reset PCIe PHY & Core, bit 22, bit 26 may be affected if write it directly  */
-    reg |= 0x00400000;
-    IFX_REG_W32(reg, IFX_RCU_RST_REQ);
-}
-
-static inline void pcie_core_rst_deassert(int pcie_port)
-{
-    u32 reg;
-
-    /* Make sure one micro-second delay */
-    udelay(1);
-
-    /* Reset PCIe PHY & Core, bit 22 */
-    reg = IFX_REG_R32(IFX_RCU_RST_REQ);
-    reg &= ~0x00400000;
-    IFX_REG_W32(reg, IFX_RCU_RST_REQ);
-}
-
-static inline void pcie_phy_rst_assert(int pcie_port)
-{
-    u32 reg;
-
-    reg = IFX_REG_R32(IFX_RCU_RST_REQ);
-    reg |= 0x00001000; /* Bit 12 */
-    IFX_REG_W32(reg, IFX_RCU_RST_REQ);
-}
-
-static inline void pcie_phy_rst_deassert(int pcie_port)
-{
-    u32 reg;
-
-    /* Make sure one micro-second delay */
-    udelay(1);
-
-    reg = IFX_REG_R32(IFX_RCU_RST_REQ);
-    reg &= ~0x00001000; /* Bit 12 */
-    IFX_REG_W32(reg, IFX_RCU_RST_REQ);
-}
-
-static inline void pcie_device_rst_assert(int pcie_port)
-{
-	gpio_set_value(IFX_PCIE_GPIO_RESET, 0);
-//    ifx_gpio_output_clear(IFX_PCIE_GPIO_RESET, ifx_pcie_gpio_module_id);
-}
-
-static inline void pcie_device_rst_deassert(int pcie_port)
-{
-    mdelay(100);
-	gpio_direction_output(IFX_PCIE_GPIO_RESET, 1);
-//    gpio_set_value(IFX_PCIE_GPIO_RESET, 1);
-    //ifx_gpio_output_set(IFX_PCIE_GPIO_RESET, ifx_pcie_gpio_module_id);
-}
-
 static inline void pcie_core_pmu_setup(int pcie_port)
 {
 	struct clk *clk;
--- a/arch/mips/pci/Makefile
+++ b/arch/mips/pci/Makefile
@@ -43,7 +43,7 @@ obj-$(CONFIG_PCI_LANTIQ)	+= pci-lantiq.o
 obj-$(CONFIG_SOC_MT7620)	+= pci-mt7620.o
 obj-$(CONFIG_SOC_RT288X)	+= pci-rt2880.o
 obj-$(CONFIG_SOC_RT3883)	+= pci-rt3883.o
-obj-$(CONFIG_PCIE_LANTIQ)	+= ifxmips_pcie_phy.o ifxmips_pcie.o fixup-lantiq-pcie.o
+obj-$(CONFIG_PCIE_LANTIQ)	+= ifxmips_pcie.o fixup-lantiq-pcie.o
 obj-$(CONFIG_PCIE_LANTIQ_MSI)	+= pcie-lantiq-msi.o
 obj-$(CONFIG_TANBAC_TB0219)	+= fixup-tb0219.o
 obj-$(CONFIG_TANBAC_TB0226)	+= fixup-tb0226.o
