From 9fb90ae6cae7f8fe4fbf626945f32cd9da2c3892 Mon Sep 17 00:00:00 2001
From: =?UTF-8?q?Rafa=C5=82=20Mi=C5=82ecki?= <rafal@milecki.pl>
Date: Mon, 20 Sep 2021 16:10:23 +0200
Subject: [PATCH] ARM: dts: BCM53573: Describe on-SoC BCM53125 rev 4 switch
MIME-Version: 1.0
Content-Type: text/plain; charset=UTF-8
Content-Transfer-Encoding: 8bit

BCM53573 family SoC have Ethernet switch connected to the first Ethernet
controller (accessible over MDIO).

Signed-off-by: Rafał Miłecki <rafal@milecki.pl>
Signed-off-by: Florian Fainelli <f.fainelli@gmail.com>
---
 arch/arm/boot/dts/bcm53573.dtsi | 18 ++++++++++++++++++
 1 file changed, 18 insertions(+)

--- a/arch/arm/boot/dts/bcm53573.dtsi
+++ b/arch/arm/boot/dts/bcm53573.dtsi
@@ -180,6 +180,24 @@
 
 		gmac0: ethernet@5000 {
 			reg = <0x5000 0x1000>;
+
+			mdio {
+				#address-cells = <1>;
+				#size-cells = <0>;
+
+				switch: switch@1e {
+					compatible = "brcm,bcm53125";
+					reg = <0x1e>;
+
+					status = "disabled";
+
+					/* ports are defined in board DTS */
+					ports {
+						#address-cells = <1>;
+						#size-cells = <0>;
+					};
+				};
+			};
 		};
 
 		gmac1: ethernet@b000 {
