#include "danube.dtsi"

#include <dt-bindings/input/input.h>

/ {
	compatible = "arcadyan,arv4525pw", "lantiq,xway", "lantiq,danube";
	model = "Speedport W501V Typ A";

	chosen {
		bootargs = "console=ttyLTQ0,115200";
	};

	aliases {
		/* we dont have a power led, lets use the online led */
		led-boot = &online;
		led-failsafe = &online;

		led-dsl = &dsl;
		led-internet = &online;
		led-wifi = &wifi;
	};

	memory@0 {
		device_type = "memory";
		reg = <0x0 0x2000000>;
	};

	ath5k_eep {
		compatible = "ath5k,eeprom";
		ath,eep-flash = <&boardconfig 0x400>;
		ath,mac-offset = <0x0>;
		ath,eep-swap;
	};

	keys {
		compatible = "gpio-keys-polled";
		poll-interval = <100>;

		wps {
			label = "wps";
			gpios = <&gpio 29 GPIO_ACTIVE_LOW>;
			linux,code = <KEY_WPS_BUTTON>;
		};
		reset {
			label = "reset";
			gpios = <&gpio 30 GPIO_ACTIVE_LOW>;
			linux,code = <KEY_RESTART>;
		};
	};

	leds {
		compatible = "gpio-leds";
		fxo {
			label = "green:festnetz";
			gpios = <&gpio 4 GPIO_ACTIVE_LOW>;
		};
		fxs {
			label = "green:internet";
			gpios = <&gpio 5 GPIO_ACTIVE_LOW>;
		};
		dsl: dsl {
			label = "green:t-dsl";
			gpios = <&gpio 6 GPIO_ACTIVE_LOW>;
		};
		wifi: wifi {
			label = "green:wlan";
			gpios = <&gpio 8 GPIO_ACTIVE_LOW>;
		};
		online: online {
			label = "green:online";
			gpios = <&gpio 9 GPIO_ACTIVE_LOW>;
		};
	};
};

&gpio {
	pinctrl-names = "default";
	pinctrl-0 = <&state_default>;

	state_default: pinmux {
		pci_rst {
			lantiq,pins = "io21";
			lantiq,pull = <2>;
			lantiq,output = <1>;
		};
		relay {
			lantiq,pins = "io31";
			lantiq,output = <1>;
		};
	};
};

/* #define ARV4525PW_PHYRESET	13 */
&gsw {
	phy-mode = "mii";
	nvmem-cells = <&macaddr_boardconfig_16>;
	nvmem-cell-names = "mac-address";
};

&localbus {
	flash@0 {
		compatible = "lantiq,nor";
		bank-width = <2>;
		reg = <0 0x0 0x2000000>;

		partitions {
			compatible = "fixed-partitions";
			#address-cells = <1>;
			#size-cells = <1>;

			partition@0 {
				label = "uboot";
				reg = <0x00000 0x10000>;
				read-only;
			};

			partition@10000 {
				label = "u-boot-env";
				reg = <0x10000 0x10000>;
				read-only;
			};

			partition@20000 {
				label = "firmware";
				reg = <0x20000 0x3d0000>;
			};

			boardconfig: partition@3f0000 {
				label = "boardconfig";
				reg = <0x3f0000 0x10000>;
				read-only;
			};
		};
	};
};

&pci0 {
	status = "okay";

	pinctrl-0 = <&pci_gnt1_pins>, <&pci_req1_pins>;
	pinctrl-names = "default";

	gpio-reset = <&gpio 21 GPIO_ACTIVE_HIGH>;
};

/* #define ARV4525PW_RELAY		31 */
&vmmc {
	status = "okay";
	gpios = <&gpio 31 GPIO_ACTIVE_HIGH>;
};

&boardconfig {
	compatible = "nvmem-cells";
	#address-cells = <1>;
	#size-cells = <1>;

	macaddr_boardconfig_16: macaddr@16 {
		reg = <0x16 0x6>;
	};
};
