#include "vr9.dtsi"

#include <dt-bindings/input/input.h>
#include <dt-bindings/mips/lantiq_rcu_gphy.h>

/ {
	compatible = "arcadyan,vgv7519", "lantiq,xway", "lantiq,vr9";

	chosen {
		bootargs = "console=ttyLTQ0,115200 mem=62M vpe1_load_addr=0x83e00000 vpe1_mem=2M maxvpes=1 maxtcs=1 nosmp";
	};

	aliases {
		led-boot = &power_green;
		led-failsafe = &power_red;
		led-running = &power_green;
		led-upgrade = &power_green;

		led-dsl = &broadband_green;
		led-internet = &internet_green;
		led-wifi = &wireless_green;
	};

	memory@0 {
		device_type = "memory";
		reg = <0x0 0x4000000>;
	};

	keys {
		compatible = "gpio-keys-polled";
		poll-interval = <100>;
		reset {
			label = "reset";
			gpios = <&gpio 9 GPIO_ACTIVE_LOW>;
			linux,code = <KEY_RESTART>;
		};
		eco {
			label = "eco";
			gpios = <&gpio 41 GPIO_ACTIVE_LOW>;
			linux,code = <BTN_0>;
		};
		rfkill {
			label = "rfkill";
			gpios = <&gpio 45 GPIO_ACTIVE_LOW>;
			linux,code = <KEY_RFKILL>;
		};
		wps {
			label = "wps";
			gpios = <&gpio 10 GPIO_ACTIVE_LOW>;
			linux,code = <KEY_WPS_BUTTON>;
		};
	};

	leds {
		compatible = "gpio-leds";

		eco {
			label = "blue:eco";
			gpios = <&stp 2 GPIO_ACTIVE_LOW>;
		};
		wps_red {
			label = "red:wps";
			gpios = <&stp 3 GPIO_ACTIVE_LOW>;
		};
		wps_green {
			label = "green:wps";
			gpios = <&stp 4 GPIO_ACTIVE_LOW>;
		};
		upgrade {
			label = "blue:upgrade";
			gpios = <&stp 5 GPIO_ACTIVE_LOW>;
		};
		tv {
			label = "green:tv";
			gpios = <&stp 6 GPIO_ACTIVE_LOW>;
		};
		internet_green: internet_green {
			label = "green:internet";
			gpios = <&stp 7 GPIO_ACTIVE_LOW>;
		};
		internet_red {
			label = "red:internet";
			gpios = <&stp 8 GPIO_ACTIVE_LOW>;
		};
		broadband_red {
			label = "red:broadband";
			gpios = <&stp 9 GPIO_ACTIVE_LOW>;
		};
		broadband_green: broadband_green {
			label = "green:broadband";
			gpios = <&stp 10 GPIO_ACTIVE_LOW>;
		};
		voice {
			label = "green:voice";
			gpios = <&stp 11 GPIO_ACTIVE_LOW>;
		};
		wireless_red {
			label = "red:wireless";
			gpios = <&stp 12 GPIO_ACTIVE_LOW>;
		};
		wireless_green: wireless_green {
			label = "green:wireless";
			gpios = <&stp 13 GPIO_ACTIVE_LOW>;
		};
		power_green: power2 {
			label = "green:power";
			gpios = <&stp 14 GPIO_ACTIVE_LOW>;
			default-state = "keep";
		};
		power_red: power {
			label = "red:power";
			gpios = <&stp 15 GPIO_ACTIVE_LOW>;
		};
	};

	usb_vbus: regulator-usb-vbus {
		compatible = "regulator-fixed";

		regulator-name = "USB_VBUS";

		regulator-min-microvolt = <5000000>;
		regulator-max-microvolt = <5000000>;

		gpio = <&gpio 32 GPIO_ACTIVE_HIGH>;
		enable-active-high;
	};
};

&eth0 {
	nvmem-cells = <&macaddr_boardconfig_16>;
	nvmem-cell-names = "mac-address";
	mac-address-increment = <1>;
};

&gphy0 {
	lantiq,gphy-mode = <GPHY_MODE_GE>;
};

&gphy1 {
	lantiq,gphy-mode = <GPHY_MODE_GE>;
};

&gpio {
	pinctrl-names = "default";
	pinctrl-0 = <&state_default>;

	state_default: pinmux {
		pci-rst {
			lantiq,pins = "io21";
			lantiq,open-drain = <0>;
			lantiq,pull = <0>;
			lantiq,output = <1>;
		};
	};
};

&gswip {
	pinctrl-0 = <&mdio_pins>, <&gphy0_led1_pins>, <&gphy1_led0_pins>;
	pinctrl-names = "default";
};

&gswip_mdio {
	phy0: ethernet-phy@0 {
		reg = <0x0>;
	};
	phy1: ethernet-phy@1 {
		reg = <0x1>;
	};
	phy5: ethernet-phy@5 {
		reg = <0x5>;
	};
	phy11: ethernet-phy@11 {
		reg = <0x11>;
	};
	phy13: ethernet-phy@13 {
		reg = <0x13>;
	};
};

&gswip_ports {
	port@0 {
		reg = <0>;
		label = "lan4";
		phy-mode = "rgmii";
		phy-handle = <&phy0>;
	};
	port@1 {
		reg = <1>;
		label = "lan3";
		phy-mode = "rgmii";
		phy-handle = <&phy1>;
	};
	port@2 {
		reg = <2>;
		label = "lan2";
		phy-mode = "internal";
		phy-handle = <&phy11>;
	};
	port@4 {
		reg = <4>;
		label = "lan1";
		phy-mode = "internal";
		phy-handle = <&phy13>;
	};
	port@5 {
		reg = <5>;
		label = "wan";
		phy-mode = "rgmii";
		phy-handle = <&phy5>;
	};
};

&localbus {
	flash@0 {
		compatible = "lantiq,nor";
		bank-width = <2>;
		reg = <0 0x0 0x800000>, <1 0x800000 0x800000>;

		partitions {
			compatible = "fixed-partitions";
			#address-cells = <1>;
			#size-cells = <1>;

			boardconfig: partition@40000 {
				label = "board_config";
				reg = <0x40000 0x10000>;
				read-only;
			};
		};
	};
};

&pci0 {
	status = "okay";
	gpio-reset = <&gpio 21 GPIO_ACTIVE_HIGH>;

	wifi@1814,3091 {
		compatible = "pci1814,3091";
		reg = <0x7000 0 0 0 0>;
		ralink,mtd-eeprom = <&boardconfig 0x410>;
		ralink,mtd-eeprom-swap;
		nvmem-cells = <&macaddr_boardconfig_16>;
		nvmem-cell-names = "mac-address";
		mac-address-increment = <1>;
	};
};

&pcie0 {
	status = "disabled";
};

&stp {
	status = "okay";
	lantiq,shadow = <0xffff>;
	lantiq,groups = <0x3>;
	/* lantiq,rising; */
};

&usb_phy0 {
	status = "okay";
};

&usb_phy1 {
	status = "okay";
};

&usb0 {
	status = "okay";
	vbus-supply = <&usb_vbus>;
};

&usb1 {
	status = "okay";
	vbus-supply = <&usb_vbus>;
};

&vmmc {
	status = "okay";
	gpios = <&gpio 30 GPIO_ACTIVE_HIGH  //fxs relay
		 &gpio 31 GPIO_ACTIVE_HIGH  //still unknown
		 &gpio 3  GPIO_ACTIVE_HIGH>; //reset_slic?
};

&boardconfig {
	compatible = "nvmem-cells";
	#address-cells = <1>;
	#size-cells = <1>;

	macaddr_boardconfig_16: macaddr@16 {
		reg = <0x16 0x6>;
	};
};
