#
# Copyright (C) 2011-2015 OpenWrt.org
#

. /lib/functions/leds.sh
. /lib/functions/uci-defaults.sh

board_config_update

led_wifi="$(get_dt_led wifi)"
[ -n "$led_wifi" ] && ucidef_set_led_wlan "wifi" "wifi" "$led_wifi" "phy0tpt"

led_dsl="$(get_dt_led dsl)"
[ -n "$led_dsl" ] && {
	led_internet="$(get_dt_led internet)"
	if [ -n "$led_internet" ]; then
		ucidef_set_led_default "dsl" "dsl" "$led_dsl" "0"
		ucidef_set_led_netdev "internet" "internet" "$led_internet" "pppoe-wan"
	else
		ucidef_set_led_netdev "dsl" "dsl" "$led_dsl" "dsl0"
	fi
}

board=$(board_name)

case "$board" in
arcadyan,arv7519rw22)
	ucidef_set_led_netdev "lan" "lan" "green:lan" "eth0.1"
	;;
arcadyan,vgv7510kw22-nor|\
arcadyan,vgv7510kw22-brn|\
zyxel,p-2812hnu-f1|\
zyxel,p-2812hnu-f3)
	ucidef_set_led_wlan "wifi" "wifi" "green:wlan" "phy0radio"
	;;
arcadyan,vgv7519-nor|\
arcadyan,vgv7519-brn)
	ucidef_set_led_wlan "wifi" "wifi" "green:wireless" "phy0radio"
	;;
avm,fritz3370-rev2-hynix|\
avm,fritz3370-rev2-micron|\
avm,fritz3390)
	ucidef_set_led_switch "lan" "LAN" "green:lan" "switch0" "0x17"
	;;
bt,homehub-v5a)
	ucidef_set_led_default "dimmed" "dimmed" "dimmed" "0"
	;;
buffalo,wbmr-300hpd)
	ucidef_set_led_switch "lan1" "LAN1" "green:lan1" "switch0" "0x08"
	ucidef_set_led_switch "lan2" "LAN2" "green:lan2" "switch0" "0x04"
	ucidef_set_led_switch "wan" "WAN" "green:wan" "switch0" "0x10"
	ucidef_set_led_switch "lan3" "LAN3" "green:lan3" "switch0" "0x20"
	ucidef_set_led_default "router" "router" "green:router" "1"
	;;
netgear,dm200)
	ucidef_set_led_netdev "lan" "lan" "green:lan" "eth0"
	;;
esac

board_config_flush

exit 0
