From patchwork Thu Feb  6 17:19:41 2020
Content-Type: text/plain; charset="utf-8"
MIME-Version: 1.0
Content-Transfer-Encoding: 7bit
X-Patchwork-Submitter: Daniel Golle <daniel@makrotopia.org>
X-Patchwork-Id: 1234465
Date: Thu, 6 Feb 2020 19:19:41 +0200
From: Daniel Golle <daniel@makrotopia.org>
To: linux-mtd@lists.infradead.org
Subject: [PATCH v2] mtd: spi-nor: Add support for xt25f128b chip
Message-ID: <20200206171941.GA2398@makrotopia.org>
MIME-Version: 1.0
Content-Disposition: inline
List-Subscribe: <http://lists.infradead.org/mailman/listinfo/linux-mtd>,
 <mailto:linux-mtd-request@lists.infradead.org?subject=subscribe>
Cc: Eitan Cohen <eitan@neot-semadar.com>, Piotr Dymacz <pepe2k@gmail.com>,
 Tudor Ambarus <tudor.ambarus@microchip.com>
Sender: "linux-mtd" <linux-mtd-bounces@lists.infradead.org>
Errors-To: linux-mtd-bounces+incoming=patchwork.ozlabs.org@lists.infradead.org

Add XT25F128B made by XTX Technology (Shenzhen) Limited.
This chip supports dual and quad read and uniform 4K-byte erase.
Verified on Teltonika RUT955 which comes with XT25F128B in recent
versions of the device.

Signed-off-by: Daniel Golle <daniel@makrotopia.org>
Signed-off-by: Felix Fietkau <nbd@nbd.name>
---
 drivers/mtd/spi-nor/spi-nor.c | 4 ++++
 1 file changed, 4 insertions(+)

--- a/drivers/mtd/spi-nor/Makefile
+++ b/drivers/mtd/spi-nor/Makefile
@@ -17,6 +17,7 @@ spi-nor-objs			+= sst.o
 spi-nor-objs			+= winbond.o
 spi-nor-objs			+= xilinx.o
 spi-nor-objs			+= xmc.o
+spi-nor-objs			+= xtx.o
 obj-$(CONFIG_MTD_SPI_NOR)	+= spi-nor.o
 
 obj-$(CONFIG_MTD_SPI_NOR)	+= controllers/
--- /dev/null
+++ b/drivers/mtd/spi-nor/xtx.c
@@ -0,0 +1,15 @@
+// SPDX-License-Identifier: GPL-2.0
+#include <linux/mtd/spi-nor.h>
+
+#include "core.h"
+
+static const struct flash_info xtx_parts[] = {
+	/* XTX Technology (Shenzhen) Limited */
+	{ "xt25f128b", INFO(0x0B4018, 0, 64 * 1024, 256, SECT_4K | SPI_NOR_DUAL_READ | SPI_NOR_QUAD_READ) },
+};
+
+const struct spi_nor_manufacturer spi_nor_xtx = {
+	.name = "xtx",
+	.parts = xtx_parts,
+	.nparts = ARRAY_SIZE(xtx_parts),
+};
--- a/drivers/mtd/spi-nor/core.c
+++ b/drivers/mtd/spi-nor/core.c
@@ -2026,6 +2026,7 @@ static const struct spi_nor_manufacturer
 	&spi_nor_winbond,
 	&spi_nor_xilinx,
 	&spi_nor_xmc,
+	&spi_nor_xtx,
 };
 
 static const struct flash_info *
--- a/drivers/mtd/spi-nor/core.h
+++ b/drivers/mtd/spi-nor/core.h
@@ -398,6 +398,7 @@ extern const struct spi_nor_manufacturer
 extern const struct spi_nor_manufacturer spi_nor_winbond;
 extern const struct spi_nor_manufacturer spi_nor_xilinx;
 extern const struct spi_nor_manufacturer spi_nor_xmc;
+extern const struct spi_nor_manufacturer spi_nor_xtx;
 
 int spi_nor_write_enable(struct spi_nor *nor);
 int spi_nor_write_disable(struct spi_nor *nor);
