From 983d96a9116a328668601555d96736261d33170c Mon Sep 17 00:00:00 2001
From: =?UTF-8?q?Rafa=C5=82=20Mi=C5=82ecki?= <rafal@milecki.pl>
Date: Thu, 16 Sep 2021 14:03:51 +0200
Subject: [PATCH] net: dsa: b53: Include all ports in "enabled_ports"
MIME-Version: 1.0
Content-Type: text/plain; charset=UTF-8
Content-Transfer-Encoding: 8bit

Make "enabled_ports" bitfield contain all available switch ports
including a CPU port. This way there is no need for fixup during
initialization.

For BCM53010, BCM53018 and BCM53019 include also other available ports.

Signed-off-by: Rafał Miłecki <rafal@milecki.pl>
Reviewed-by: Florian Fainelli <f.fainelli@gmail.com>
Tested-by: Florian Fainelli <f.fainelli@gmail.com>
Signed-off-by: Jakub Kicinski <kuba@kernel.org>
---
 drivers/net/dsa/b53/b53_common.c | 23 +++++++++++------------
 1 file changed, 11 insertions(+), 12 deletions(-)

--- a/drivers/net/dsa/b53/b53_common.c
+++ b/drivers/net/dsa/b53/b53_common.c
@@ -2288,7 +2288,7 @@ static const struct b53_chip_data b53_sw
 		.chip_id = BCM5325_DEVICE_ID,
 		.dev_name = "BCM5325",
 		.vlans = 16,
-		.enabled_ports = 0x1f,
+		.enabled_ports = 0x3f,
 		.arl_bins = 2,
 		.arl_buckets = 1024,
 		.imp_port = 5,
@@ -2299,7 +2299,7 @@ static const struct b53_chip_data b53_sw
 		.chip_id = BCM5365_DEVICE_ID,
 		.dev_name = "BCM5365",
 		.vlans = 256,
-		.enabled_ports = 0x1f,
+		.enabled_ports = 0x3f,
 		.arl_bins = 2,
 		.arl_buckets = 1024,
 		.imp_port = 5,
@@ -2310,7 +2310,7 @@ static const struct b53_chip_data b53_sw
 		.chip_id = BCM5389_DEVICE_ID,
 		.dev_name = "BCM5389",
 		.vlans = 4096,
-		.enabled_ports = 0x1f,
+		.enabled_ports = 0x11f,
 		.arl_bins = 4,
 		.arl_buckets = 1024,
 		.imp_port = 8,
@@ -2324,7 +2324,7 @@ static const struct b53_chip_data b53_sw
 		.chip_id = BCM5395_DEVICE_ID,
 		.dev_name = "BCM5395",
 		.vlans = 4096,
-		.enabled_ports = 0x1f,
+		.enabled_ports = 0x11f,
 		.arl_bins = 4,
 		.arl_buckets = 1024,
 		.imp_port = 8,
@@ -2338,7 +2338,7 @@ static const struct b53_chip_data b53_sw
 		.chip_id = BCM5397_DEVICE_ID,
 		.dev_name = "BCM5397",
 		.vlans = 4096,
-		.enabled_ports = 0x1f,
+		.enabled_ports = 0x11f,
 		.arl_bins = 4,
 		.arl_buckets = 1024,
 		.imp_port = 8,
@@ -2352,7 +2352,7 @@ static const struct b53_chip_data b53_sw
 		.chip_id = BCM5398_DEVICE_ID,
 		.dev_name = "BCM5398",
 		.vlans = 4096,
-		.enabled_ports = 0x7f,
+		.enabled_ports = 0x17f,
 		.arl_bins = 4,
 		.arl_buckets = 1024,
 		.imp_port = 8,
@@ -2366,7 +2366,7 @@ static const struct b53_chip_data b53_sw
 		.chip_id = BCM53115_DEVICE_ID,
 		.dev_name = "BCM53115",
 		.vlans = 4096,
-		.enabled_ports = 0x1f,
+		.enabled_ports = 0x11f,
 		.arl_bins = 4,
 		.arl_buckets = 1024,
 		.vta_regs = B53_VTA_REGS,
@@ -2380,7 +2380,7 @@ static const struct b53_chip_data b53_sw
 		.chip_id = BCM53125_DEVICE_ID,
 		.dev_name = "BCM53125",
 		.vlans = 4096,
-		.enabled_ports = 0xff,
+		.enabled_ports = 0x1ff,
 		.arl_bins = 4,
 		.arl_buckets = 1024,
 		.imp_port = 8,
@@ -2422,7 +2422,7 @@ static const struct b53_chip_data b53_sw
 		.chip_id = BCM53010_DEVICE_ID,
 		.dev_name = "BCM53010",
 		.vlans = 4096,
-		.enabled_ports = 0x1f,
+		.enabled_ports = 0x1bf,
 		.arl_bins = 4,
 		.arl_buckets = 1024,
 		.imp_port = 8,
@@ -2464,7 +2464,7 @@ static const struct b53_chip_data b53_sw
 		.chip_id = BCM53018_DEVICE_ID,
 		.dev_name = "BCM53018",
 		.vlans = 4096,
-		.enabled_ports = 0x1f,
+		.enabled_ports = 0x1bf,
 		.arl_bins = 4,
 		.arl_buckets = 1024,
 		.imp_port = 8,
@@ -2478,7 +2478,7 @@ static const struct b53_chip_data b53_sw
 		.chip_id = BCM53019_DEVICE_ID,
 		.dev_name = "BCM53019",
 		.vlans = 4096,
-		.enabled_ports = 0x1f,
+		.enabled_ports = 0x1bf,
 		.arl_bins = 4,
 		.arl_buckets = 1024,
 		.imp_port = 8,
@@ -2605,7 +2605,6 @@ static int b53_switch_init(struct b53_de
 			dev->cpu_port = 5;
 	}
 
-	dev->enabled_ports |= BIT(dev->cpu_port);
 	dev->num_ports = fls(dev->enabled_ports);
 
 	dev->ds->num_ports = min_t(unsigned int, dev->num_ports, DSA_MAX_PORTS);
