#
# Copyright (C) 2015 OpenWrt.org
#

. /lib/functions/uci-defaults.sh

board_config_update

board=$(board_name)

case "$board" in
traverse,ls1043v)
	ucidef_add_gpio_switch "lte_reset" "LTE Reset" "377"
	ucidef_add_gpio_switch "lte_disable" "LTE Airplane mode" "378"
	;;
traverse,ls1043s)
	ucidef_add_gpio_switch "tensfp_txdisable" "SFP+ TX Disable" "378"
	ucidef_add_gpio_switch "gigsfp_txdisable" "SFP TX Disable" "381"
	ucidef_add_gpio_switch "lte_reset" "LTE Reset" "502"
	ucidef_add_gpio_switch "lte_disable" "LTE Airplane Mode" "394"
	ucidef_add_gpio_switch "lte_power" "LTE Power" "395"
	;;
esac

board_config_flush

exit 0
