From a40da00390f47fa698ef9ef9a2c82d427f6f8aa6 Mon Sep 17 00:00:00 2001
From: Alex Marginean <alexandru.marginean@nxp.com>
Date: Tue, 7 Jan 2020 16:44:20 +0200
Subject: [PATCH] drivers: net: felix: set link based on BMSR, not LPA

At least some PHYs don't advertise link up during system side AN, rely on
local indication from internal PHYs for link state.

Signed-off-by: Alex Marginean <alexandru.marginean@nxp.com>
---
 drivers/net/dsa/ocelot/felix_vsc9959.c | 1 -
 1 file changed, 1 deletion(-)

--- a/drivers/net/dsa/ocelot/felix_vsc9959.c
+++ b/drivers/net/dsa/ocelot/felix_vsc9959.c
@@ -896,7 +896,6 @@ static void vsc9959_pcs_link_state_usxgm
 		break;
 	}
 
-	pcs->link = USXGMII_LPA_LNKS(lpa);
 	if (USXGMII_LPA_DUPLEX(lpa))
 		pcs->duplex = DUPLEX_FULL;
 	else
