#include "rt3883.dtsi"

#include <dt-bindings/gpio/gpio.h>
#include <dt-bindings/input/input.h>

/ {
	compatible = "trendnet,tew-692gr", "ralink,rt3883-soc";
	model = "TRENDnet TEW-692GR";

	aliases {
		led-boot = &led_wps_green;
		led-failsafe = &led_wps_green;
		led-running = &led_wps_green;
		led-upgrade = &led_wps_green;
	};

	flash@1c000000 {
		compatible = "cfi-flash";
		reg = <0x1c000000 0x800000>;
		bank-width = <2>;

		partitions {
			compatible = "fixed-partitions";
			#address-cells = <1>;
			#size-cells = <1>;

			partition@0 {
				reg = <0x0 0x0030000>;
				label = "u-boot";
				read-only;
			};

			partition@30000 {
				reg = <0x00030000 0x00010000>;
				label = "u-boot-env";
				read-only;
			};

			factory: partition@40000 {
				reg = <0x00040000 0x00010000>;
				label = "factory";
				read-only;
			};

			partition@50000 {
				compatible = "denx,uimage";
				reg = <0x00050000 0x007b0000>;
				label = "firmware";
			};
		};
	};

	keys {
		compatible = "gpio-keys-polled";
		poll-interval = <100>;

		reset {
			label = "reset";
			gpios = <&gpio0 10 GPIO_ACTIVE_LOW>;
			linux,code = <KEY_RESTART>;
		};

		wps {
			label = "wps";
			gpios = <&gpio1 2 GPIO_ACTIVE_LOW>;
			linux,code = <KEY_WPS_BUTTON>;
		};
	};

	leds {
		compatible = "gpio-leds";

		wps {
			label = "orange:wps";
			gpios = <&gpio0 9 GPIO_ACTIVE_LOW>;
		};

		led_wps_green: wps2 {
			label = "green:wps";
			gpios = <&gpio1 4 GPIO_ACTIVE_LOW>;
		};
	};
};

&gpio1 {
	status = "okay";
};

&state_default {
	gpio {
		groups = "spi", "i2c", "jtag", "uartf";
		function = "gpio";
	};
};

&ethernet {
	status = "okay";
	nvmem-cells = <&macaddr_factory_4>;
	nvmem-cell-names = "mac-address";

	port@0 {
		phy-handle = <&phy0>;
		phy-mode = "rgmii";
	};

	mdio-bus {
		status = "okay";

		phy0: ethernet-phy@0 {
			reg = <0>;
			phy-mode = "rgmii";

			qca,ar8327-initvals = <
				0x04 0x07600000 /* PORT0 PAD MODE CTRL */
				0x0c 0x07600000 /* PORT6 PAD MODE CTRL */
				0x10 0x40000000 /* Power-on Strapping: 176-pin interface configuration */
				0x50 0xc437c437 /* LED Control Register 0 */
				0x54 0xc337c337 /* LED Control Register 1 */
				0x58 0x00000000 /* LED Control Register 2 */
				0x5c 0x03ffff00 /* LED Control Register 3 */
				0x7c 0x0000007e /* PORT0_STATUS */
				0x94 0x0000007e /* PORT6 STATUS */
			>;
		};
	};
};

&pci {
	status = "okay";
};

&pci1 {
	status = "okay";

	wifi@0,0 {
		compatible = "pci0,0";
		reg = < 0x10000 0 0 0 0 >;
		ralink,2ghz = <0>;
	};
};

&wmac {
	status = "okay";
	ralink,mtd-eeprom = <&factory 0x0>;
	ralink,5ghz = <0>;
	nvmem-cells = <&macaddr_factory_4>;
	nvmem-cell-names = "mac-address";
	mac-address-increment = <3>;
};

&factory {
	compatible = "nvmem-cells";
	#address-cells = <1>;
	#size-cells = <1>;

	macaddr_factory_4: macaddr@4 {
		reg = <0x4 0x6>;
	};
};
