From a9c640d91233d2e1b38e32644a5f53bc2de1fce0 Mon Sep 17 00:00:00 2001
From: Maxime Ripard <maxime@cerno.tech>
Date: Thu, 29 Apr 2021 21:58:27 +0200
Subject: [PATCH] drm/vc4: hdmi: Simplify the connector state retrieval

When we have the entire DRM state, retrieving the connector state only
requires the drm_connector pointer. Fortunately for us, we have
allocated it as a part of the vc4_hdmi structure, so we can retrieve get
a pointer by simply accessing our field in that structure.

Signed-off-by: Maxime Ripard <maxime@cerno.tech>
---
 drivers/gpu/drm/vc4/vc4_hdmi.c | 21 +++------------------
 1 file changed, 3 insertions(+), 18 deletions(-)

--- a/drivers/gpu/drm/vc4/vc4_hdmi.c
+++ b/drivers/gpu/drm/vc4/vc4_hdmi.c
@@ -851,31 +851,16 @@ static void vc4_hdmi_recenter_fifo(struc
 		  "VC4_HDMI_FIFO_CTL_RECENTER_DONE");
 }
 
-static struct drm_connector_state *
-vc4_hdmi_encoder_get_connector_state(struct drm_encoder *encoder,
-				     struct drm_atomic_state *state)
-{
-	struct drm_connector_state *conn_state;
-	struct drm_connector *connector;
-	unsigned int i;
-
-	for_each_new_connector_in_state(state, connector, conn_state, i) {
-		if (conn_state->best_encoder == encoder)
-			return conn_state;
-	}
-
-	return NULL;
-}
-
 static void vc4_hdmi_encoder_pre_crtc_configure(struct drm_encoder *encoder,
 						struct drm_atomic_state *state)
 {
+	struct vc4_hdmi *vc4_hdmi = encoder_to_vc4_hdmi(encoder);
+	struct drm_connector *connector = &vc4_hdmi->connector;
 	struct drm_connector_state *conn_state =
-		vc4_hdmi_encoder_get_connector_state(encoder, state);
+		drm_atomic_get_new_connector_state(state, connector);
 	struct vc4_hdmi_connector_state *vc4_conn_state =
 		conn_state_to_vc4_hdmi_conn_state(conn_state);
 	struct drm_display_mode *mode = &encoder->crtc->state->adjusted_mode;
-	struct vc4_hdmi *vc4_hdmi = encoder_to_vc4_hdmi(encoder);
 	unsigned long bvb_rate, pixel_rate, hsm_rate;
 	int ret;
 
