// SPDX-License-Identifier: GPL-2.0-or-later

#include "qcom-ipq4019.dtsi"
#include <dt-bindings/gpio/gpio.h>
#include <dt-bindings/input/input.h>
#include <dt-bindings/soc/qcom,tcsr.h>

/ {
	model = "EnGenius EMD1";
	compatible = "engenius,emd1";

	aliases {
		led-boot = &led_power;
		led-failsafe = &led_power;
		led-running = &led_power;
		led-upgrade = &led_power;
	};

	soc {
		rng@22000 {
			status = "okay";
		};

		mdio@90000 {
			status = "okay";
		};

		ess-psgmii@98000 {
			status = "okay";
		};

		tcsr@1949000 {
			compatible = "qcom,tcsr";
			reg = <0x1949000 0x100>;
			qcom,wifi_glb_cfg = <TCSR_WIFI_GLB_CFG>;
		};

		ess_tcsr@1953000 {
			compatible = "qcom,tcsr";
			reg = <0x1953000 0x1000>;
			qcom,ess-interface-select = <TCSR_ESS_PSGMII>;
		};

		tcsr@1957000 {
			compatible = "qcom,tcsr";
			reg = <0x1957000 0x100>;
			qcom,wifi_noc_memtype_m0_m2 = <TCSR_WIFI_NOC_MEMTYPE_M0_M2>;
		};

		crypto@8e3a000 {
			status = "okay";
		};

		watchdog@b017000 {
			status = "okay";
		};

		ess-switch@c000000 {
			status = "okay";
			switch_lan_bmp = <0x20>;
			switch_wan_bmp = <0x00>;
		};

		edma@c080000 {
			status = "okay";
			qcom,num_gmac = <1>;
		};
	};

	keys {
		compatible = "gpio-keys";

		reset {
			label = "reset";
			gpios = <&tlmm 63 GPIO_ACTIVE_LOW>;
			linux,code = <KEY_RESTART>;
		};
	};

	leds {
		compatible = "gpio-leds";

		led_power: power {
			label = "white:power";
			gpios = <&tlmm 58 GPIO_ACTIVE_LOW>;
		};

		wlan2g {
			label = "red:wlan2g";
			gpios = <&tlmm 2 GPIO_ACTIVE_HIGH>;
			linux,default-trigger = "phy0tpt";
		};

		wlan5g {
			label = "blue:wlan5g";
			gpios = <&tlmm 3 GPIO_ACTIVE_HIGH>;
			linux,default-trigger = "phy1tpt";
		};

		mesh {
			label = "orange:mesh";
			gpios = <&tlmm 0 GPIO_ACTIVE_HIGH>;
		};
	};
};

&tlmm {
	serial_pins: serial_pinmux {
		mux {
			pins = "gpio60", "gpio61";
			function = "blsp_uart0";
			bias-disable;
		};
	};

	spi_0_pins: spi_0_pinmux {
		pin {
			function = "blsp_spi0";
			pins = "gpio54", "gpio55", "gpio56", "gpio57";
			drive-strength = <12>;
			bias-disable;
		};

		pin_cs {
			function = "gpio";
			pins = "gpio54";
			drive-strength = <2>;
			bias-disable;
			output-high;
		};
	};
};

&blsp_dma {
	status = "okay";
};

&blsp1_spi1 {
	pinctrl-0 = <&spi_0_pins>;
	pinctrl-names = "default";
	status = "okay";
	cs-gpios = <&tlmm 54 GPIO_ACTIVE_HIGH>;

	flash@0 {
		compatible = "jedec,spi-nor";
		reg = <0>;
		spi-max-frequency = <24000000>;
		partitions {
			compatible = "fixed-partitions";
			#address-cells = <1>;
			#size-cells = <1>;

			partition0@0 {
				label = "0:SBL1";
				reg = <0x00000000 0x00040000>;
				read-only;
			};
			partition1@40000 {
				label = "0:MIBIB";
				reg = <0x00040000 0x00020000>;
				read-only;
			};
			partition2@60000 {
				label = "0:QSEE";
				reg = <0x00060000 0x00060000>;
				read-only;
			};
			partition3@c0000 {
				label = "0:CDT";
				reg = <0x000c0000 0x00010000>;
				read-only;
			};
			partition4@d0000 {
				label = "0:DDRPARAMS";
				reg = <0x000d0000 0x00010000>;
				read-only;
			};
			partition5@e0000 {
				label = "0:APPSBLENV";
				reg = <0x000e0000 0x00010000>;
				read-only;
			};
			partition6@f0000 {
				label = "0:APPSBL";
				reg = <0x000f0000 0x00080000>;
				read-only;
			};
			partition7@170000 {
				label = "0:ART";
				reg = <0x00170000 0x00010000>;
				read-only;
			};
			partition8@180000 {
				label = "userconfig";
				reg = <0x00180000 0x00080000>;
				read-only;
			};
			partition9@200000 {
				compatible = "denx,fit";
				label = "firmware";
				reg = <0x200000 0x01e00000>;
			};
		};
	};
};

&blsp1_uart1 {
	pinctrl-0 = <&serial_pins>;
	pinctrl-names = "default";
	status = "okay";
};

&gmac0 {
	qcom,phy_mdio_addr = <4>;
	qcom,poll_required = <1>;
	qcom,forced_speed = <1000>;
	qcom,forced_duplex = <1>;
	vlan_tag = <1 0x20>;
};

&cryptobam {
	status = "okay";
};

&wifi0 {
	status = "okay";
	qcom,ath10k-calibration-variant = "EnGenius-EMD1";
};

&wifi1 {
	status = "okay";
	qcom,ath10k-calibration-variant = "EnGenius-EMD1";
};
