From d6988cf1d16faac56899918bb2b1be8d85155e3f Mon Sep 17 00:00:00 2001
From: =?UTF-8?q?=C3=81lvaro=20Fern=C3=A1ndez=20Rojas?= <noltari@gmail.com>
Date: Sat, 20 Feb 2021 18:36:38 +0100
Subject: [PATCH] hwrng: bcm2835: set quality to 1000
MIME-Version: 1.0
Content-Type: text/plain; charset=UTF-8
Content-Transfer-Encoding: 8bit

This allows devices without a high precission timer to reduce boot from >100s
to <30s.

Signed-off-by: Álvaro Fernández Rojas <noltari@gmail.com>
---
 drivers/char/hw_random/bcm2835-rng.c | 1 +
 1 file changed, 1 insertion(+)

--- a/drivers/char/hw_random/bcm2835-rng.c
+++ b/drivers/char/hw_random/bcm2835-rng.c
@@ -167,6 +167,7 @@ static int bcm2835_rng_probe(struct plat
 	priv->rng.init = bcm2835_rng_init;
 	priv->rng.read = bcm2835_rng_read;
 	priv->rng.cleanup = bcm2835_rng_cleanup;
+	priv->rng.quality = 1000;
 
 	if (dev_of_node(dev)) {
 		rng_id = of_match_node(bcm2835_rng_of_match, np);
