From 4da57dbbffdfa7fe4e2b70b047fc5ff95ff25a3d Mon Sep 17 00:00:00 2001
From: =?UTF-8?q?=C3=81lvaro=20Fern=C3=A1ndez=20Rojas?= <noltari@gmail.com>
Date: Tue, 23 Feb 2021 18:44:55 +0100
Subject: [PATCH 3/3] usb: host: ehci-platform: add spurious_oc DT support
MIME-Version: 1.0
Content-Type: text/plain; charset=UTF-8
Content-Transfer-Encoding: 8bit

Over-current reporting isn't supported on some platforms such as bcm63xx.
These devices will incorrectly report over-current if this flag isn't properly
activated.

Signed-off-by: Álvaro Fernández Rojas <noltari@gmail.com>
Link: https://lore.kernel.org/r/20210223174455.1378-4-noltari@gmail.com
Signed-off-by: Greg Kroah-Hartman <gregkh@linuxfoundation.org>
---
 drivers/usb/host/ehci-platform.c | 3 +++
 1 file changed, 3 insertions(+)

--- a/drivers/usb/host/ehci-platform.c
+++ b/drivers/usb/host/ehci-platform.c
@@ -286,6 +286,9 @@ static int ehci_platform_probe(struct pl
 		if (of_property_read_bool(dev->dev.of_node, "big-endian"))
 			ehci->big_endian_mmio = ehci->big_endian_desc = 1;
 
+		if (of_property_read_bool(dev->dev.of_node, "spurious-oc"))
+			ehci->spurious_oc = 1;
+
 		if (of_property_read_bool(dev->dev.of_node,
 					  "needs-reset-on-resume"))
 			priv->reset_on_resume = true;
