// SPDX-License-Identifier: GPL-2.0-or-later OR MIT

#include "mt7621.dtsi"

#include <dt-bindings/gpio/gpio.h>
#include <dt-bindings/input/input.h>

/ {
	aliases {
		led-boot = &led_power_orange;
		led-failsafe = &led_power_green;
		led-running = &led_power_green;
		led-upgrade = &led_net_orange;
	};

	keys {
		compatible = "gpio-keys";

		reset {
			label = "reset";
			gpios = <&gpio 15 GPIO_ACTIVE_LOW>;
			linux,code = <KEY_RESTART>;
		};

		wps {
			label = "wps";
			gpios = <&gpio 18 GPIO_ACTIVE_LOW>;
			linux,code = <KEY_WPS_BUTTON>;
		};

		wifi {
			label = "wifi";
			gpios = <&gpio 7 GPIO_ACTIVE_LOW>;
			linux,code = <KEY_RFKILL>;
		};
	};

	leds: leds {
		compatible = "gpio-leds";

		led_power_orange: power_orange {
			label = "orange:power";
			gpios = <&gpio 8 GPIO_ACTIVE_LOW>;
		};

		led_power_green: power_green {
			label = "green:power";
			gpios = <&gpio 16 GPIO_ACTIVE_LOW>;
		};

		led_net_orange: net_orange {
			label = "orange:net";
			gpios = <&gpio 4 GPIO_ACTIVE_LOW>;
		};

		net_green {
			label = "green:net";
			gpios = <&gpio 3 GPIO_ACTIVE_LOW>;
		};
	};
};

&pcie {
	status = "okay";
};

&pcie0 {
	wifi@0,0 {
		compatible = "mediatek,mt76";
		reg = <0x0000 0 0 0 0>;
		mediatek,mtd-eeprom = <&factory 0x0000>;
		ieee80211-freq-limit = <2400000 2500000>;

		led {
			led-active-low;
		};
	};
};

&pcie1 {
	wifi@0,0 {
		compatible = "mediatek,mt76";
		reg = <0x0000 0 0 0 0>;
		mediatek,mtd-eeprom = <&factory 0x8000>;
		ieee80211-freq-limit = <5000000 6000000>;

		led {
			led-active-low;
		};
	};
};

&switch0 {
	ports {
		port@0 {
			status = "okay";
			label = "lan4";
		};

		port@1 {
			status = "okay";
			label = "lan3";
		};

		port@2 {
			status = "okay";
			label = "lan2";
		};

		port@3 {
			status = "okay";
			label = "lan1";
		};

		wan: port@4 {
			status = "okay";
			label = "wan";
		};
	};
};

&state_default {
	gpio {
		groups = "i2c", "uart3", "jtag", "wdt";
		function = "gpio";
	};
};
