From effbf244f11642594a739755285cd16591831b13 Mon Sep 17 00:00:00 2001
From: Markus Proeller <markus.proeller@pieye.org>
Date: Thu, 10 Oct 2019 19:12:08 +0200
Subject: [PATCH] dt-bindings: Add binding for the Infineon IRS1125
 sensor

Adds a binding for the Infineon IRS1125 time-of-flight depth
sensor.

Signed-off-by: Markus Proeller <markus.proeller@pieye.org>
---
 .../devicetree/bindings/media/i2c/irs1125.txt | 48 +++++++++++++++++++
 1 file changed, 48 insertions(+)
 create mode 100644 Documentation/devicetree/bindings/media/i2c/irs1125.txt

--- /dev/null
+++ b/Documentation/devicetree/bindings/media/i2c/irs1125.txt
@@ -0,0 +1,48 @@
+* Infineon irs1125 time of flight sensor
+
+The Infineon irs1125 is a time of flight digital image sensor with
+an active array size of 352H x 286V. It is programmable through I2C
+interface. The I2C address defaults to 0x3D, but can be reconfigured
+to address 0x3C or 0x41 via I2C commands. Image data is sent through
+MIPI CSI-2, which is configured as either 1 or 2 data lanes.
+
+Required Properties:
+- compatible: value should be "infineon,irs1125" for irs1125 sensor
+- reg: I2C bus address of the device
+- clocks: reference to the xclk input clock.
+- pwdn-gpios: reference to the GPIO connected to the reset pin.
+	      This is an active low signal to the iirs1125.
+
+The irs1125 device node should contain one 'port' child node with
+an 'endpoint' subnode. For further reading on port node refer to
+Documentation/devicetree/bindings/media/video-interfaces.txt.
+
+Endpoint node required properties for CSI-2 connection are:
+- remote-endpoint: a phandle to the bus receiver's endpoint node.
+- clock-lanes: should be set to <0> (clock lane on hardware lane 0)
+- data-lanes: should be set to <1> or <1 2> (one or two lane CSI-2
+  supported)
+
+Example:
+	sensor@10 {
+		compatible = "infineon,irs1125";
+		reg = <0x3D>;
+		#address-cells = <1>;
+		#size-cells = <0>;
+		clocks = <&irs1125_clk>;
+		pwdn-gpios = <&gpio 5 0>;
+
+		irs1125_clk: camera-clk {
+			compatible = "fixed-clock";
+			#clock-cells = <0>;
+			clock-frequency = <26000000>;
+		};
+
+		port {
+			sensor_out: endpoint {
+				remote-endpoint = <&csiss_in>;
+				clock-lanes = <0>;
+				data-lanes = <1 2>;
+			};
+		};
+	};
