From eac607290fee8b1bcd08c48ac49f089f41a0e696 Mon Sep 17 00:00:00 2001
From: Phil Elwell <phil@raspberrypi.org>
Date: Wed, 29 May 2019 15:47:42 +0100
Subject: [PATCH] arm: bcm2835: DMA can only address 1GB

The legacy peripherals can only address the first gigabyte of RAM, so
ensure that DMA allocations are restricted to that region.

Signed-off-by: Phil Elwell <phil@raspberrypi.org>
---
 arch/arm/mach-bcm/board_bcm2835.c | 3 +++
 1 file changed, 3 insertions(+)

--- a/arch/arm/mach-bcm/board_bcm2835.c
+++ b/arch/arm/mach-bcm/board_bcm2835.c
@@ -114,6 +114,9 @@ static const char * const bcm2835_compat
 };
 
 DT_MACHINE_START(BCM2835, "BCM2835")
+#if defined(CONFIG_ZONE_DMA) && defined(CONFIG_ARM_LPAE)
+	.dma_zone_size	= SZ_1G,
+#endif
 	.map_io = bcm2835_map_io,
 	.init_machine = bcm2835_init,
 	.dt_compat = bcm2835_compat,
