From fa817272c37ef78e25dc14e4760ac78a7043a18a Mon Sep 17 00:00:00 2001
From: Felix Fietkau <nbd@nbd.name>
Date: Thu, 22 Apr 2021 22:21:07 -0700
Subject: [PATCH] net: ethernet: mtk_eth_soc: set PPE flow hash as skb hash if
 present

This improves GRO performance

Signed-off-by: Felix Fietkau <nbd@nbd.name>
[Ilya: Use MTK_RXD4_FOE_ENTRY instead of GENMASK(13, 0)]
Signed-off-by: Ilya Lipnitskiy <ilya.lipnitskiy@gmail.com>
Signed-off-by: David S. Miller <davem@davemloft.net>
---
 drivers/net/ethernet/mediatek/mtk_eth_soc.c | 8 ++++++++
 1 file changed, 8 insertions(+)

--- a/drivers/net/ethernet/mediatek/mtk_eth_soc.c
+++ b/drivers/net/ethernet/mediatek/mtk_eth_soc.c
@@ -19,6 +19,7 @@
 #include <linux/interrupt.h>
 #include <linux/pinctrl/devinfo.h>
 #include <linux/phylink.h>
+#include <linux/jhash.h>
 #include <net/dsa.h>
 
 #include "mtk_eth_soc.h"
@@ -1271,6 +1272,7 @@ static int mtk_poll_rx(struct napi_struc
 		struct net_device *netdev;
 		unsigned int pktlen;
 		dma_addr_t dma_addr;
+		u32 hash;
 		int mac;
 
 		ring = mtk_get_rx_ring(eth);
@@ -1340,6 +1342,12 @@ static int mtk_poll_rx(struct napi_struc
 		skb->protocol = eth_type_trans(skb, netdev);
 		bytes += pktlen;
 
+		hash = trxd.rxd4 & MTK_RXD4_FOE_ENTRY;
+		if (hash != MTK_RXD4_FOE_ENTRY) {
+			hash = jhash_1word(hash, 0);
+			skb_set_hash(skb, hash, PKT_HASH_TYPE_L4);
+		}
+
 		if (netdev->features & NETIF_F_HW_VLAN_CTAG_RX &&
 		    (trxd.rxd2 & RX_DMA_VTAG))
 			__vlan_hwaccel_put_tag(skb, htons(ETH_P_8021Q),
