From 078ced30af696b52a450a016a16eb47499d68117 Mon Sep 17 00:00:00 2001
From: Linus Walleij <linus.walleij@linaro.org>
Date: Wed, 8 Jul 2020 14:25:36 +0200
Subject: [PATCH 2/5] net: dsa: tag_rtl4_a: Implement Realtek 4 byte A tag

This implements the known parts of the Realtek 4 byte
tag protocol version 0xA, as found in the RTL8366RB
DSA switch.

It is designated as protocol version 0xA as a
different Realtek 4 byte tag format with protocol
version 0x9 is known to exist in the Realtek RTL8306
chips.

The tag and switch chip lacks public documentation, so
the tag format has been reverse-engineered from
packet dumps. As only ingress traffic has been available
for analysis an egress tag has not been possible to
develop (even using educated guesses about bit fields)
so this is as far as it gets. It is not known if the
switch even supports egress tagging.

Excessive attempts to figure out the egress tag format
was made. When nothing else worked, I just tried all bit
combinations with 0xannp where a is protocol and p is
port. I looped through all values several times trying
to get a response from ping, without any positive
result.

Using just these ingress tags however, the switch
functionality is vastly improved and the packets find
their way into the destination port without any
tricky VLAN configuration. On the D-Link DIR-685 the
LAN ports now come up and respond to ping without
any command line configuration so this is a real
improvement for users.

Egress packets need to be restricted to the proper
target ports using VLAN, which the RTL8366RB DSA
switch driver already sets up.

Cc: DENG Qingfang <dqfext@gmail.com>
Cc: Mauri Sandberg <sandberg@mailfence.com>
Reviewed-by: Andrew Lunn <andrew@lunn.ch>
Reviewed-by: Florian Fainelli <f.fainelli@gmail.com>
Signed-off-by: Linus Walleij <linus.walleij@linaro.org>
Signed-off-by: David S. Miller <davem@davemloft.net>
---
 include/net/dsa.h    |   2 +
 net/dsa/Kconfig      |   7 +++
 net/dsa/Makefile     |   1 +
 net/dsa/tag_rtl4_a.c | 130 +++++++++++++++++++++++++++++++++++++++++++
 4 files changed, 140 insertions(+)
 create mode 100644 net/dsa/tag_rtl4_a.c

--- a/include/net/dsa.h
+++ b/include/net/dsa.h
@@ -42,6 +42,7 @@ struct phylink_link_state;
 #define DSA_TAG_PROTO_8021Q_VALUE		12
 #define DSA_TAG_PROTO_SJA1105_VALUE		13
 #define DSA_TAG_PROTO_KSZ8795_VALUE		14
+#define DSA_TAG_PROTO_RTL4_A_VALUE		17
 
 enum dsa_tag_protocol {
 	DSA_TAG_PROTO_NONE		= DSA_TAG_PROTO_NONE_VALUE,
@@ -59,6 +60,7 @@ enum dsa_tag_protocol {
 	DSA_TAG_PROTO_8021Q		= DSA_TAG_PROTO_8021Q_VALUE,
 	DSA_TAG_PROTO_SJA1105		= DSA_TAG_PROTO_SJA1105_VALUE,
 	DSA_TAG_PROTO_KSZ8795		= DSA_TAG_PROTO_KSZ8795_VALUE,
+	DSA_TAG_PROTO_RTL4_A		= DSA_TAG_PROTO_RTL4_A_VALUE,
 };
 
 struct packet_type;
--- a/net/dsa/Kconfig
+++ b/net/dsa/Kconfig
@@ -80,6 +80,13 @@ config NET_DSA_TAG_KSZ
 	  Say Y if you want to enable support for tagging frames for the
 	  Microchip 8795/9477/9893 families of switches.
 
+config NET_DSA_TAG_RTL4_A
+	tristate "Tag driver for Realtek 4 byte protocol A tags"
+	help
+	  Say Y or M if you want to enable support for tagging frames for the
+	  Realtek switches with 4 byte protocol A tags, sich as found in
+	  the Realtek RTL8366RB.
+
 config NET_DSA_TAG_QCA
 	tristate "Tag driver for Qualcomm Atheros QCA8K switches"
 	help
--- a/net/dsa/Makefile
+++ b/net/dsa/Makefile
@@ -10,6 +10,7 @@ obj-$(CONFIG_NET_DSA_TAG_DSA) += tag_dsa
 obj-$(CONFIG_NET_DSA_TAG_EDSA) += tag_edsa.o
 obj-$(CONFIG_NET_DSA_TAG_GSWIP) += tag_gswip.o
 obj-$(CONFIG_NET_DSA_TAG_KSZ) += tag_ksz.o
+obj-$(CONFIG_NET_DSA_TAG_RTL4_A) += tag_rtl4_a.o
 obj-$(CONFIG_NET_DSA_TAG_LAN9303) += tag_lan9303.o
 obj-$(CONFIG_NET_DSA_TAG_MTK) += tag_mtk.o
 obj-$(CONFIG_NET_DSA_TAG_QCA) += tag_qca.o
--- /dev/null
+++ b/net/dsa/tag_rtl4_a.c
@@ -0,0 +1,130 @@
+// SPDX-License-Identifier: GPL-2.0
+/*
+ * Handler for Realtek 4 byte DSA switch tags
+ * Currently only supports protocol "A" found in RTL8366RB
+ * Copyright (c) 2020 Linus Walleij <linus.walleij@linaro.org>
+ *
+ * This "proprietary tag" header looks like so:
+ *
+ * -------------------------------------------------
+ * | MAC DA | MAC SA | 0x8899 | 2 bytes tag | Type |
+ * -------------------------------------------------
+ *
+ * The 2 bytes tag form a 16 bit big endian word. The exact
+ * meaning has been guessed from packet dumps from ingress
+ * frames, as no working egress traffic has been available
+ * we do not know the format of the egress tags or if they
+ * are even supported.
+ */
+
+#include <linux/etherdevice.h>
+#include <linux/bits.h>
+
+#include "dsa_priv.h"
+
+#define RTL4_A_HDR_LEN		4
+#define RTL4_A_ETHERTYPE	0x8899
+#define RTL4_A_PROTOCOL_SHIFT	12
+/*
+ * 0x1 = Realtek Remote Control protocol (RRCP)
+ * 0x2/0x3 seems to be used for loopback testing
+ * 0x9 = RTL8306 DSA protocol
+ * 0xa = RTL8366RB DSA protocol
+ */
+#define RTL4_A_PROTOCOL_RTL8366RB	0xa
+
+static struct sk_buff *rtl4a_tag_xmit(struct sk_buff *skb,
+				      struct net_device *dev)
+{
+	/*
+	 * Just let it pass thru, we don't know if it is possible
+	 * to tag a frame with the 0x8899 ethertype and direct it
+	 * to a specific port, all attempts at reverse-engineering have
+	 * ended up with the frames getting dropped.
+	 *
+	 * The VLAN set-up needs to restrict the frames to the right port.
+	 *
+	 * If you have documentation on the tagging format for RTL8366RB
+	 * (tag type A) then please contribute.
+	 */
+	return skb;
+}
+
+static struct sk_buff *rtl4a_tag_rcv(struct sk_buff *skb,
+				     struct net_device *dev,
+				     struct packet_type *pt)
+{
+	u16 protport;
+	__be16 *p;
+	u16 etype;
+	u8 *tag;
+	u8 prot;
+	u8 port;
+
+	if (unlikely(!pskb_may_pull(skb, RTL4_A_HDR_LEN)))
+		return NULL;
+
+	/* The RTL4 header has its own custom Ethertype 0x8899 and that
+	 * starts right at the beginning of the packet, after the src
+	 * ethernet addr. Apparantly skb->data always points 2 bytes in,
+	 * behind the Ethertype.
+	 */
+	tag = skb->data - 2;
+	p = (__be16 *)tag;
+	etype = ntohs(*p);
+	if (etype != RTL4_A_ETHERTYPE) {
+		/* Not custom, just pass through */
+		netdev_dbg(dev, "non-realtek ethertype 0x%04x\n", etype);
+		return skb;
+	}
+	p = (__be16 *)(tag + 2);
+	protport = ntohs(*p);
+	/* The 4 upper bits are the protocol */
+	prot = (protport >> RTL4_A_PROTOCOL_SHIFT) & 0x0f;
+	if (prot != RTL4_A_PROTOCOL_RTL8366RB) {
+		netdev_err(dev, "unknown realtek protocol 0x%01x\n", prot);
+		return NULL;
+	}
+	port = protport & 0xff;
+
+	skb->dev = dsa_master_find_slave(dev, 0, port);
+	if (!skb->dev) {
+		netdev_dbg(dev, "could not find slave for port %d\n", port);
+		return NULL;
+	}
+
+	/* Remove RTL4 tag and recalculate checksum */
+	skb_pull_rcsum(skb, RTL4_A_HDR_LEN);
+
+	/* Move ethernet DA and SA in front of the data */
+	memmove(skb->data - ETH_HLEN,
+		skb->data - ETH_HLEN - RTL4_A_HDR_LEN,
+		2 * ETH_ALEN);
+
+	skb->offload_fwd_mark = 1;
+
+	return skb;
+}
+
+static int rtl4a_tag_flow_dissect(const struct sk_buff *skb, __be16 *proto,
+				  int *offset)
+{
+	*offset = RTL4_A_HDR_LEN;
+	/* Skip past the tag and fetch the encapsulated Ethertype */
+	*proto = ((__be16 *)skb->data)[1];
+
+	return 0;
+}
+
+static const struct dsa_device_ops rtl4a_netdev_ops = {
+	.name	= "rtl4a",
+	.proto	= DSA_TAG_PROTO_RTL4_A,
+	.xmit	= rtl4a_tag_xmit,
+	.rcv	= rtl4a_tag_rcv,
+	.flow_dissect = rtl4a_tag_flow_dissect,
+	.overhead = RTL4_A_HDR_LEN,
+};
+module_dsa_tag_driver(rtl4a_netdev_ops);
+
+MODULE_LICENSE("GPL");
+MODULE_ALIAS_DSA_TAG_DRIVER(DSA_TAG_PROTO_RTL4_A);
