From c6faef087c0a9a5f89dd29e1a557cb3dfc4b993b Mon Sep 17 00:00:00 2001
From: Dom Cobley <popcornmix@gmail.com>
Date: Wed, 6 Jan 2021 18:16:29 +0000
Subject: [PATCH] bcm2711-rpi.dtsi: Bump hdmi audio dma panic priority
 to max

Set panic priority to 15 and leave normal priority at 0

Signed-off-by: Dom Cobley <popcornmix@gmail.com>
---
 arch/arm/boot/dts/bcm2711-rpi.dtsi | 4 ++--
 1 file changed, 2 insertions(+), 2 deletions(-)

--- a/arch/arm/boot/dts/bcm2711-rpi.dtsi
+++ b/arch/arm/boot/dts/bcm2711-rpi.dtsi
@@ -179,7 +179,7 @@
 };
 
 &hdmi0 {
-	dmas = <&dma (10|(1<<27)|(1<<24))>;
+	dmas = <&dma (10|(1<<27)|(1<<24)|(0<<16)|(15<<20))>;
 	status = "disabled";
 };
 
@@ -188,7 +188,7 @@
 };
 
 &hdmi1 {
-	dmas = <&dma (17|(1<<27)|(1<<24))>;
+	dmas = <&dma (17|(1<<27)|(1<<24)|(0<<16)|(15<<20))>;
 	status = "disabled";
 };
 
