From 319fb2652bdfc0176ec8c69ce612c0f0dcc4a0ed Mon Sep 17 00:00:00 2001
From: popcornmix <popcornmix@gmail.com>
Date: Mon, 11 Jan 2021 14:49:33 +0000
Subject: [PATCH] bcm2835-dma: Move WAIT_RESP from extra to info

Questionable: Might want to drop
Signed-off-by: popcornmix <popcornmix@gmail.com>
---
 drivers/dma/bcm2835-dma.c | 4 ++--
 1 file changed, 2 insertions(+), 2 deletions(-)

--- a/drivers/dma/bcm2835-dma.c
+++ b/drivers/dma/bcm2835-dma.c
@@ -861,9 +861,9 @@ static struct dma_async_tx_descriptor *b
 {
 	struct bcm2835_chan *c = to_bcm2835_dma_chan(chan);
 	struct bcm2835_desc *d;
-	u32 info = BCM2835_DMA_D_INC | BCM2835_DMA_S_INC |
+	u32 info = BCM2835_DMA_D_INC | BCM2835_DMA_S_INC | WAIT_RESP(c->dreq) |
 		   WIDE_SOURCE(c->dreq) | WIDE_DEST(c->dreq);
-	u32 extra = BCM2835_DMA_INT_EN | WAIT_RESP(c->dreq);
+	u32 extra = BCM2835_DMA_INT_EN;
 	size_t max_len = bcm2835_dma_max_frame_length(c);
 	size_t frames;
 
