From: =?UTF-8?q?Rafa=C5=82=20Mi=C5=82ecki?= <rafal@milecki.pl>
Subject: [PATCH] ARM: dts: BCM5301X: Specify switch ports for remaining
 devices
MIME-Version: 1.0
Content-Type: text/plain; charset=UTF-8
Content-Transfer-Encoding: 8bit

Signed-off-by: Rafał Miłecki <rafal@milecki.pl>
---

--- a/arch/arm/boot/dts/bcm4708-asus-rt-ac56u.dts
+++ b/arch/arm/boot/dts/bcm4708-asus-rt-ac56u.dts
@@ -93,3 +93,40 @@
 &usb3_phy {
 	status = "okay";
 };
+
+&srab {
+	status = "okay";
+
+	ports {
+		port@0 {
+			reg = <0>;
+			label = "lan1";
+		};
+
+		port@1 {
+			reg = <1>;
+			label = "lan2";
+		};
+
+		port@2 {
+			reg = <2>;
+			label = "lan3";
+		};
+
+		port@3 {
+			reg = <3>;
+			label = "lan4";
+		};
+
+		port@4 {
+			reg = <4>;
+			label = "wan";
+		};
+
+		port@5 {
+			reg = <5>;
+			label = "cpu";
+			ethernet = <&gmac0>;
+		};
+	};
+};
--- a/arch/arm/boot/dts/bcm4708-asus-rt-ac68u.dts
+++ b/arch/arm/boot/dts/bcm4708-asus-rt-ac68u.dts
@@ -83,3 +83,40 @@
 &usb3_phy {
 	status = "okay";
 };
+
+&srab {
+	status = "okay";
+
+	ports {
+		port@0 {
+			reg = <0>;
+			label = "wan";
+		};
+
+		port@1 {
+			reg = <1>;
+			label = "lan1";
+		};
+
+		port@2 {
+			reg = <2>;
+			label = "lan2";
+		};
+
+		port@3 {
+			reg = <3>;
+			label = "lan3";
+		};
+
+		port@4 {
+			reg = <4>;
+			label = "lan4";
+		};
+
+		port@5 {
+			reg = <5>;
+			label = "cpu";
+			ethernet = <&gmac0>;
+		};
+	};
+};
--- a/arch/arm/boot/dts/bcm4708-buffalo-wzr-1750dhp.dts
+++ b/arch/arm/boot/dts/bcm4708-buffalo-wzr-1750dhp.dts
@@ -149,3 +149,40 @@
 &usb3_phy {
 	status = "okay";
 };
+
+&srab {
+	status = "okay";
+
+	ports {
+		port@0 {
+			reg = <0>;
+			label = "lan1";
+		};
+
+		port@1 {
+			reg = <1>;
+			label = "lan2";
+		};
+
+		port@2 {
+			reg = <2>;
+			label = "lan3";
+		};
+
+		port@3 {
+			reg = <3>;
+			label = "lan4";
+		};
+
+		port@4 {
+			reg = <4>;
+			label = "wan";
+		};
+
+		port@5 {
+			reg = <5>;
+			label = "cpu";
+			ethernet = <&gmac0>;
+		};
+	};
+};
--- a/arch/arm/boot/dts/bcm4708-linksys-ea6300-v1.dts
+++ b/arch/arm/boot/dts/bcm4708-linksys-ea6300-v1.dts
@@ -46,3 +46,40 @@
 &usb3_phy {
 	status = "okay";
 };
+
+&srab {
+	status = "okay";
+
+	ports {
+		port@0 {
+			reg = <0>;
+			label = "lan1";
+		};
+
+		port@1 {
+			reg = <1>;
+			label = "lan2";
+		};
+
+		port@2 {
+			reg = <2>;
+			label = "lan3";
+		};
+
+		port@3 {
+			reg = <3>;
+			label = "lan4";
+		};
+
+		port@4 {
+			reg = <4>;
+			label = "wan";
+		};
+
+		port@5 {
+			reg = <5>;
+			label = "cpu";
+			ethernet = <&gmac0>;
+		};
+	};
+};
--- a/arch/arm/boot/dts/bcm4708-linksys-ea6500-v2.dts
+++ b/arch/arm/boot/dts/bcm4708-linksys-ea6500-v2.dts
@@ -42,3 +42,40 @@
 &usb3_phy {
 	status = "okay";
 };
+
+&srab {
+	status = "okay";
+
+	ports {
+		port@0 {
+			reg = <0>;
+			label = "lan1";
+		};
+
+		port@1 {
+			reg = <1>;
+			label = "lan2";
+		};
+
+		port@2 {
+			reg = <2>;
+			label = "lan3";
+		};
+
+		port@3 {
+			reg = <3>;
+			label = "lan4";
+		};
+
+		port@4 {
+			reg = <4>;
+			label = "wan";
+		};
+
+		port@5 {
+			reg = <5>;
+			label = "cpu";
+			ethernet = <&gmac0>;
+		};
+	};
+};
--- a/arch/arm/boot/dts/bcm4708-netgear-r6300-v2.dts
+++ b/arch/arm/boot/dts/bcm4708-netgear-r6300-v2.dts
@@ -86,3 +86,40 @@
 &usb3_phy {
 	status = "okay";
 };
+
+&srab {
+	status = "okay";
+
+	ports {
+		port@0 {
+			reg = <0>;
+			label = "lan1";
+		};
+
+		port@1 {
+			reg = <1>;
+			label = "lan2";
+		};
+
+		port@2 {
+			reg = <2>;
+			label = "lan3";
+		};
+
+		port@3 {
+			reg = <3>;
+			label = "lan4";
+		};
+
+		port@4 {
+			reg = <4>;
+			label = "wan";
+		};
+
+		port@5 {
+			reg = <5>;
+			label = "cpu";
+			ethernet = <&gmac0>;
+		};
+	};
+};
--- a/arch/arm/boot/dts/bcm47081-asus-rt-n18u.dts
+++ b/arch/arm/boot/dts/bcm47081-asus-rt-n18u.dts
@@ -77,3 +77,40 @@
 &usb3_phy {
 	status = "okay";
 };
+
+&srab {
+	status = "okay";
+
+	ports {
+		port@0 {
+			reg = <0>;
+			label = "wan";
+		};
+
+		port@1 {
+			reg = <1>;
+			label = "lan1";
+		};
+
+		port@2 {
+			reg = <2>;
+			label = "lan2";
+		};
+
+		port@3 {
+			reg = <3>;
+			label = "lan3";
+		};
+
+		port@4 {
+			reg = <4>;
+			label = "lan4";
+		};
+
+		port@5 {
+			reg = <5>;
+			label = "cpu";
+			ethernet = <&gmac0>;
+		};
+	};
+};
--- a/arch/arm/boot/dts/bcm4709-asus-rt-ac87u.dts
+++ b/arch/arm/boot/dts/bcm4709-asus-rt-ac87u.dts
@@ -68,6 +68,38 @@
 	status = "okay";
 };
 
+&srab {
+	status = "okay";
+
+	ports {
+		port@0 {
+			reg = <0>;
+			label = "wan";
+		};
+
+		port@1 {
+			reg = <1>;
+			label = "lan1";
+		};
+
+		port@2 {
+			reg = <2>;
+			label = "lan2";
+		};
+
+		port@3 {
+			reg = <3>;
+			label = "lan3";
+		};
+
+		port@7 {
+			reg = <7>;
+			label = "cpu";
+			ethernet = <&gmac1>;
+		};
+	};
+};
+
 &nandcs {
 	partitions {
 		compatible = "fixed-partitions";
--- a/arch/arm/boot/dts/bcm4709-buffalo-wxr-1900dhp.dts
+++ b/arch/arm/boot/dts/bcm4709-buffalo-wxr-1900dhp.dts
@@ -132,3 +132,40 @@
 &usb3_phy {
 	status = "okay";
 };
+
+&srab {
+	status = "okay";
+
+	ports {
+		port@0 {
+			reg = <0>;
+			label = "lan1";
+		};
+
+		port@1 {
+			reg = <1>;
+			label = "lan2";
+		};
+
+		port@2 {
+			reg = <2>;
+			label = "lan3";
+		};
+
+		port@3 {
+			reg = <3>;
+			label = "lan4";
+		};
+
+		port@4 {
+			reg = <4>;
+			label = "wan";
+		};
+
+		port@5 {
+			reg = <5>;
+			label = "cpu";
+			ethernet = <&gmac0>;
+		};
+	};
+};
--- a/arch/arm/boot/dts/bcm4709-linksys-ea9200.dts
+++ b/arch/arm/boot/dts/bcm4709-linksys-ea9200.dts
@@ -49,3 +49,45 @@
 &usb3_phy {
 	status = "okay";
 };
+
+&srab {
+	status = "okay";
+
+	ports {
+		port@0 {
+			reg = <0>;
+			label = "lan1";
+		};
+
+		port@1 {
+			reg = <1>;
+			label = "lan2";
+		};
+
+		port@2 {
+			reg = <2>;
+			label = "lan3";
+		};
+
+		port@3 {
+			reg = <3>;
+			label = "lan4";
+		};
+
+		port@4 {
+			reg = <4>;
+			label = "wan";
+		};
+
+		port@8 {
+			reg = <8>;
+			label = "cpu";
+			ethernet = <&gmac2>;
+
+			fixed-link {
+				speed = <1000>;
+				full-duplex;
+			};
+		};
+	};
+};
--- a/arch/arm/boot/dts/bcm4709-netgear-r7000.dts
+++ b/arch/arm/boot/dts/bcm4709-netgear-r7000.dts
@@ -106,3 +106,40 @@
 &usb3_phy {
 	status = "okay";
 };
+
+&srab {
+	status = "okay";
+
+	ports {
+		port@0 {
+			reg = <0>;
+			label = "wan";
+		};
+
+		port@1 {
+			reg = <1>;
+			label = "lan1";
+		};
+
+		port@2 {
+			reg = <2>;
+			label = "lan2";
+		};
+
+		port@3 {
+			reg = <3>;
+			label = "lan3";
+		};
+
+		port@4 {
+			reg = <4>;
+			label = "lan4";
+		};
+
+		port@5 {
+			reg = <5>;
+			label = "cpu";
+			ethernet = <&gmac0>;
+		};
+	};
+};
--- a/arch/arm/boot/dts/bcm47094-netgear-r8500.dts
+++ b/arch/arm/boot/dts/bcm47094-netgear-r8500.dts
@@ -94,3 +94,45 @@
 &usb3_phy {
 	status = "okay";
 };
+
+&srab {
+	status = "okay";
+
+	ports {
+		port@0 {
+			reg = <0>;
+			label = "wan";
+		};
+
+		port@1 {
+			reg = <1>;
+			label = "lan1";
+		};
+
+		port@2 {
+			reg = <2>;
+			label = "lan2";
+		};
+
+		port@3 {
+			reg = <3>;
+			label = "lan3";
+		};
+
+		port@4 {
+			reg = <4>;
+			label = "lan4";
+		};
+
+		port@8 {
+			reg = <8>;
+			label = "cpu";
+			ethernet = <&gmac2>;
+
+			fixed-link {
+				speed = <1000>;
+				full-duplex;
+			};
+		};
+	};
+};
--- a/arch/arm/boot/dts/bcm47094-phicomm-k3.dts
+++ b/arch/arm/boot/dts/bcm47094-phicomm-k3.dts
@@ -38,6 +38,38 @@
 	status = "okay";
 };
 
+&srab {
+	status = "okay";
+
+	ports {
+		port@0 {
+			reg = <0>;
+			label = "lan1";
+		};
+
+		port@1 {
+			reg = <1>;
+			label = "lan2";
+		};
+
+		port@2 {
+			reg = <2>;
+			label = "lan3";
+		};
+
+		port@3 {
+			reg = <3>;
+			label = "wan";
+		};
+
+		port@5 {
+			reg = <5>;
+			label = "cpu";
+			ethernet = <&gmac0>;
+		};
+	};
+};
+
 &nandcs {
 	partitions {
 		compatible = "fixed-partitions";
