// SPDX-License-Identifier: GPL-2.0-or-later OR MIT

#include "mt7621.dtsi"

#include <dt-bindings/gpio/gpio.h>
#include <dt-bindings/input/input.h>

/ {
	compatible = "zyxel,wap6805", "mediatek,mt7621-soc";
	model = "ZyXEL WAP6805";

	aliases {
		led-boot = &led_status_green;
		led-failsafe = &led_status_red;
		led-running = &led_status_green;
		led-upgrade = &led_status_green;
		label-mac-device = &gmac0;
	};

	leds {
		compatible = "gpio-leds";

		led_status_red: status_red {
			label = "red:status";
			gpios = <&gpio 4 GPIO_ACTIVE_HIGH>;
		};

		status_blink {
			label = "blink:status";
			gpios = <&gpio 7 GPIO_ACTIVE_HIGH>;
		};

		led_status_green: status_green {
			label = "green:status";
			gpios = <&gpio 13 GPIO_ACTIVE_HIGH>;
		};
	};

	keys {
		compatible = "gpio-keys";

		wps {
			label = "wps";
			gpios = <&gpio 8 GPIO_ACTIVE_LOW>;
			linux,code = <KEY_WPS_BUTTON>;
		};

		reset {
			label = "reset";
			gpios = <&gpio 18 GPIO_ACTIVE_LOW>;
			linux,code = <KEY_RESTART>;
		};
	};
};

&nand {
	status = "okay";

	partitions {
		compatible = "fixed-partitions";
		#address-cells = <1>;
		#size-cells = <1>;

		partition@0 {
			label = "Bootloader";
			reg = <0x0 0x100000>;
			read-only;
		};

		partition@100000 {
			label = "MRD";
			reg = <0x100000 0x100000>;
			read-only;
		};

		factory: partition@200000 {
			label = "Factory";
			reg = <0x200000 0x100000>;
			read-only;
		};

		partition@300000 {
			label = "Config";
			reg = <0x300000 0x100000>;
		};

		partition@400000 {
			label = "Kernel";
			reg = <0x400000 0x2000000>;
		};

		partition@800000 {
			label = "ubi";
			reg = <0x800000 0x1c00000>;
		};

		partition@2400000 {
			label = "Kernel2";
			reg = <0x2400000 0x2000000>;
		};

		partition@4400000 {
			label = "Private";
			reg = <0x4400000 0x100000>;
		};

		partition@4500000 {
			label = "Log";
			reg = <0x4500000 0x1000000>;
		};

		partition@5500000 {
			label = "App";
			reg = <0x5500000 0x2b00000>;
		};
	};
};

&pcie {
	status = "okay";
};

&pcie0 {
	mt76@0,0 {
		reg = <0x0000 0 0 0 0>;
		mediatek,mtd-eeprom = <&factory 0x0>;
	};
};

&gmac0 {
	nvmem-cells = <&macaddr_factory_e000>;
	nvmem-cell-names = "mac-address";
};

&gmac1 {
	status = "okay";

	fixed-link {
		speed = <1000>;
		full-duplex;
	};
};

&switch0 {
	ports {
		port@0 {
			status = "okay";
			label = "lan4";
		};
		port@1 {
			status = "okay";
			label = "lan3";
		};
		port@2 {
			status = "okay";
			label = "lan2";
		};
		port@3 {
			status = "okay";
			label = "lan1";
		};
	};
};

&xhci {
	status = "disabled";
};

&state_default {
	gpio {
		groups = "i2c", "uart3", "jtag", "wdt";
		function = "gpio";
	};
};

&factory {
	compatible = "nvmem-cells";
	#address-cells = <1>;
	#size-cells = <1>;

	macaddr_factory_e000: macaddr@e000 {
		reg = <0xe000 0x6>;
	};
};
