From 32fe7cc286f4a4d7f5d623ddb9fba10907c2abea Mon Sep 17 00:00:00 2001
From: Phil Elwell <phil@raspberrypi.org>
Date: Thu, 17 Dec 2015 13:37:07 +0000
Subject: [PATCH] hci_h5: Don't send conf_req when ACTIVE

Without this patch, a modem and kernel can continuously bombard each
other with conf_req and conf_rsp messages, in a demented game of tag.
---
 drivers/bluetooth/hci_h5.c | 3 ++-
 1 file changed, 2 insertions(+), 1 deletion(-)

--- a/drivers/bluetooth/hci_h5.c
+++ b/drivers/bluetooth/hci_h5.c
@@ -343,7 +343,8 @@ static void h5_handle_internal_rx(struct
 		h5_link_control(hu, conf_req, 3);
 	} else if (memcmp(data, conf_req, 2) == 0) {
 		h5_link_control(hu, conf_rsp, 2);
-		h5_link_control(hu, conf_req, 3);
+		if (h5->state != H5_ACTIVE)
+		    h5_link_control(hu, conf_req, 3);
 	} else if (memcmp(data, conf_rsp, 2) == 0) {
 		if (H5_HDR_LEN(hdr) > 2)
 			h5->tx_win = (data[2] & 0x07);
