--- /dev/null
+++ b/board/arcadyan/arv8539pw22/Makefile
@@ -0,0 +1,28 @@
+#
+# Copyright (C) 2000-2011 Wolfgang Denk, DENX Software Engineering, wd@denx.de
+#
+# SPDX-License-Identifier:     GPL-2.0+
+#
+
+include $(TOPDIR)/config.mk
+
+LIB    = $(obj)lib$(BOARD).o
+
+COBJS  = $(BOARD).o
+
+SRCS   := $(SOBJS:.o=.S) $(COBJS:.o=.c)
+OBJS   := $(addprefix $(obj),$(COBJS))
+SOBJS  := $(addprefix $(obj),$(SOBJS))
+
+$(LIB):        $(obj).depend $(OBJS) $(SOBJS)
+	$(call cmd_link_o_target, $(OBJS) $(SOBJS))
+
+#########################################################################
+
+# defines $(obj).depend target
+include $(SRCTREE)/rules.mk
+
+sinclude $(obj).depend
+
+#########################################################################
+
--- /dev/null
+++ b/board/arcadyan/arv8539pw22/arv8539pw22.c
@@ -0,0 +1,53 @@
+/*
+ * Copyright (C) 2012 Luka Perkov <luka@openwrt.org>
+ * Copyright (C) 2013 Oliver Muth <dr.o.muth@gmx.de>
+ *
+ * SPDX-License-Identifier:    GPL-2.0+
+ */
+
+#include <common.h>
+#include <switch.h>
+#include <asm/gpio.h>
+#include <asm/lantiq/eth.h>
+#include <asm/lantiq/reset.h>
+#include <asm/lantiq/chipid.h>
+
+int board_early_init_f(void)
+{
+       return 0;
+}
+
+int checkboard(void)
+{
+       puts("Board: " CONFIG_BOARD_NAME "\n");
+       ltq_chip_print_info();
+
+       return 0;
+}
+
+static const struct ltq_eth_port_config eth_port_config[] = {
+       /* MAC0: Atheros ar8216 switch */
+       { 0, 0x0, LTQ_ETH_PORT_SWITCH, PHY_INTERFACE_MODE_MII },
+};
+
+static const struct ltq_eth_board_config eth_board_config = {
+       .ports = eth_port_config,
+       .num_ports = ARRAY_SIZE(eth_port_config),
+};
+
+int board_eth_init(bd_t *bis)
+{
+       return ltq_eth_initialize(&eth_board_config);
+}
+
+static struct switch_device ar8216_dev = {
+       .name = "ar8216",
+       .cpu_port = 0,
+       .port_mask = 0xF,
+};
+
+int board_switch_init(void)
+{
+       return switch_device_register(&ar8216_dev);
+}
+
--- /dev/null
+++ b/board/arcadyan/arv8539pw22/config.mk
@@ -0,0 +1,8 @@
+#
+# Copyright (C) 2011-2013 Daniel Schwierzeck, daniel.schwierzeck@gmail.com
+#
+# SPDX-License-Identifier:     GPL-2.0+
+#
+
+PLATFORM_CPPFLAGS += -I$(TOPDIR)/board/$(BOARDDIR)
+
--- /dev/null
+++ b/board/arcadyan/arv8539pw22/ddr_settings.h
@@ -0,0 +1,55 @@
+/*
+ * Copyright (C) 2011-2013 Luka Perkov <luka@openwrt.org>
+ *
+ * This file has been generated with lantiq_ram_extract_magic.awk script.     
+ *
+ * SPDX-License-Identifier:    GPL-2.0+
+ */
+
+#define MC_DC00_VALUE  0x1B1B
+#define MC_DC01_VALUE  0x0
+#define MC_DC02_VALUE  0x0
+#define MC_DC03_VALUE  0x0
+#define MC_DC04_VALUE  0x0
+#define MC_DC05_VALUE  0x200
+#define MC_DC06_VALUE  0x605
+#define MC_DC07_VALUE  0x303
+#define MC_DC08_VALUE  0x102
+#define MC_DC09_VALUE  0x70A
+#define MC_DC10_VALUE  0x203
+#define MC_DC11_VALUE  0xC02
+#define MC_DC12_VALUE  0x1C8
+#define MC_DC13_VALUE  0x1
+#define MC_DC14_VALUE  0x0
+#define MC_DC15_VALUE  0x134
+#define MC_DC16_VALUE  0xC800
+#define MC_DC17_VALUE  0xD
+#define MC_DC18_VALUE  0x301
+#define MC_DC19_VALUE  0x200
+#define MC_DC20_VALUE  0xA03
+#define MC_DC21_VALUE  0x1400
+#define MC_DC22_VALUE  0x1414
+#define MC_DC23_VALUE  0x0
+#define MC_DC24_VALUE  0x5B
+#define MC_DC25_VALUE  0x0
+#define MC_DC26_VALUE  0x0
+#define MC_DC27_VALUE  0x0
+#define MC_DC28_VALUE  0x510
+#define MC_DC29_VALUE  0x4E20
+#define MC_DC30_VALUE  0x8235
+#define MC_DC31_VALUE  0x0
+#define MC_DC32_VALUE  0x0
+#define MC_DC33_VALUE  0x0
+#define MC_DC34_VALUE  0x0
+#define MC_DC35_VALUE  0x0
+#define MC_DC36_VALUE  0x0
+#define MC_DC37_VALUE  0x0
+#define MC_DC38_VALUE  0x0
+#define MC_DC39_VALUE  0x0
+#define MC_DC40_VALUE  0x0
+#define MC_DC41_VALUE  0x0
+#define MC_DC42_VALUE  0x0
+#define MC_DC43_VALUE  0x0
+#define MC_DC44_VALUE  0x0
+#define MC_DC45_VALUE  0x500
+#define MC_DC46_VALUE  0x0
--- a/boards.cfg
+++ b/boards.cfg
@@ -520,6 +520,9 @@ Active  mips        mips32         danub
 Active  mips        mips32         danube      arcadyan        arv752dpw22         arv752dpw22_brn                      arv752dpw22:SYS_BOOT_BRN                                                                                                          -
 Active  mips        mips32         danube      arcadyan        arv752dpw22         arv752dpw22_nor                      arv752dpw22:SYS_BOOT_NOR                                                                                                          -
 Active  mips        mips32         danube      arcadyan        arv752dpw22         arv752dpw22_ram                      arv752dpw22:SYS_BOOT_RAM                                                                                                          -
+Active  mips        mips32         danube      arcadyan        arv8539pw22         arv8539pw22_brn                      arv8539pw22:SYS_BOOT_BRN                                                                                                          -
+Active  mips        mips32         danube      arcadyan        arv8539pw22         arv8539pw22_nor                      arv8539pw22:SYS_BOOT_NOR                                                                                                          -
+Active  mips        mips32         danube      arcadyan        arv8539pw22         arv8539pw22_ram                      arv8539pw22:SYS_BOOT_RAM                                                                                                          -
 Active  mips        mips32         danube      audiocodes      acmp252             acmp252_nor                          acmp252:SYS_BOOT_NOR                                                                                                              Daniel Golle <daniel.golle@gmail.com>
 Active  mips        mips32         danube      audiocodes      acmp252             acmp252_ram                          acmp252:SYS_BOOT_RAM                                                                                                              Daniel Golle <daniel.golle@gmail.com>
 Active  mips        mips32         danube      gigaset         sx76x               gigasx76x_nor                        sx76x:SYS_BOOT_NOR                                                                                                                Luka Perkov <luka@openwrt.org>
--- /dev/null
+++ b/include/configs/arv8539pw22.h
@@ -0,0 +1,70 @@
+/*
+ * Copyright (C) 2012-2013 Luka Perkov <luka@openwrt.org>
+ *
+ * SPDX-License-Identifier:    GPL-2.0+
+ */
+
+#ifndef __CONFIG_H
+#define __CONFIG_H
+
+#define CONFIG_MACH_TYPE       "ARV8539PW22"
+#define CONFIG_IDENT_STRING    " "CONFIG_MACH_TYPE
+#define CONFIG_BOARD_NAME      "Speedport W 504V Typ A"
+
+/* Configure SoC */
+#define CONFIG_LTQ_SUPPORT_UART                /* Enable ASC and UART */
+
+#define CONFIG_LTQ_SUPPORT_ETHERNET    /* Enable ethernet */
+
+#define CONFIG_LTQ_SUPPORT_NOR_FLASH   /* Have a parallel NOR flash */
+
+#define CONFIG_SYS_BOOTM_LEN		0x1000000	/* 16 MB */
+
+/* Switch devices */
+#define CONFIG_SWITCH_MULTI
+#define CONFIG_SWITCH_AR8216
+
+/* Environment */
+#if defined(CONFIG_SYS_BOOT_NOR)
+#define CONFIG_ENV_IS_IN_FLASH
+#define CONFIG_ENV_OVERWRITE
+#define CONFIG_ENV_OFFSET              (192 * 1024)
+#define CONFIG_ENV_SECT_SIZE           (64 * 1024)
+#else
+#define CONFIG_ENV_IS_NOWHERE
+#endif
+
+#define CONFIG_ENV_SIZE                        (8 * 1024)
+#define CONFIG_LOADADDR                        CONFIG_SYS_LOAD_ADDR
+
+/* Burnboot loadable image */
+#if defined(CONFIG_SYS_BOOT_BRN)
+#define CONFIG_SYS_TEXT_BASE           0x80002000
+#define CONFIG_SKIP_LOWLEVEL_INIT
+#define CONFIG_SYS_DISABLE_CACHE
+#define CONFIG_ENV_OVERWRITE 1
+#endif
+
+
+/* Console */
+#define CONFIG_LTQ_ADVANCED_CONSOLE
+#define CONFIG_BAUDRATE                        115200
+#define CONFIG_CONSOLE_ASC             1
+#define CONFIG_CONSOLE_DEV             "ttyS1"
+
+/* Pull in default board configs for Lantiq XWAY Danube */
+#include <asm/lantiq/config.h>
+#include <asm/arch/config.h>
+
+/* Pull in default OpenWrt configs for Lantiq SoC */
+#include "openwrt-lantiq-common.h"
+
+#define CONFIG_ENV_UPDATE_UBOOT_NOR            \
+       "update-uboot-nor=run load-uboot-nor write-uboot-nor\0"
+
+#define CONFIG_EXTRA_ENV_SETTINGS      \
+       CONFIG_ENV_LANTIQ_DEFAULTS      \
+       CONFIG_ENV_UPDATE_UBOOT_NOR     \
+       "kernel_addr=0xB0040000\0"
+
+#endif /* __CONFIG_H */
