#
# Copyright (C) 2016 OpenWrt.org
#

. /lib/functions/uci-defaults.sh

board_config_update

case "$(board_name)" in
snps,axs103|\
snps,hsdk)
	ucidef_set_interface_lan "eth0" "dhcp"
	;;
esac

board_config_flush

exit 0
