From b290c6384afabbca5ae6e2af72fb1b2bc37922be Mon Sep 17 00:00:00 2001
From: =?UTF-8?q?Rafa=C5=82=20Mi=C5=82ecki?= <rafal@milecki.pl>
Date: Thu, 16 Sep 2021 14:03:52 +0200
Subject: [PATCH] net: dsa: b53: Drop BCM5301x workaround for a wrong CPU/IMP
 port
MIME-Version: 1.0
Content-Type: text/plain; charset=UTF-8
Content-Transfer-Encoding: 8bit

On BCM5301x port 8 requires a fixed link when used.

Years ago when b53 was an OpenWrt downstream driver (with configuration
based on sometimes bugged NVRAM) there was a need for a fixup. In case
of forcing fixed link for (incorrectly specified) port 5 the code had to
actually setup port 8 link.

For upstream b53 driver with setup based on DT there is no need for that
workaround. In DT we have and require correct ports setup.

Signed-off-by: Rafał Miłecki <rafal@milecki.pl>
Reviewed-by: Florian Fainelli <f.fainelli@gmail.com>
Tested-by: Florian Fainelli <f.fainelli@gmail.com>
Signed-off-by: Jakub Kicinski <kuba@kernel.org>
---
 drivers/net/dsa/b53/b53_common.c | 6 ------
 1 file changed, 6 deletions(-)

--- a/drivers/net/dsa/b53/b53_common.c
+++ b/drivers/net/dsa/b53/b53_common.c
@@ -1256,12 +1256,6 @@ static void b53_adjust_link(struct dsa_s
 				return;
 			}
 		}
-	} else if (is5301x(dev)) {
-		if (port != dev->cpu_port) {
-			b53_force_port_config(dev, dev->cpu_port, 2000,
-					      DUPLEX_FULL, true, true);
-			b53_force_link(dev, dev->cpu_port, 1);
-		}
 	}
 
 	/* Re-negotiate EEE if it was enabled already */
