/dts-v1/;

/ {
	#address-cells = <1>;
	#size-cells = <1>;
	compatible = "brcm,bcm6368";

	aliases {
		nflash = &nflash;
		pflash = &pflash;
		pinctrl = &pinctrl;
		serial0 = &uart0;
		serial1 = &uart1;
		spi0 = &lsspi;
	};

	cpus {
		#address-cells = <1>;
		#size-cells = <0>;

		cpu@0 {
			compatible = "brcm,bmips4350", "mips,mips4Kc";
			device_type = "cpu";
			reg = <0>;
		};

		cpu@1 {
			compatible = "brcm,bmips4350", "mips,mips4Kc";
			device_type = "cpu";
			reg = <1>;
		};
	};

	cpu_intc: interrupt-controller {
		#address-cells = <0>;
		compatible = "mti,cpu-interrupt-controller";

		interrupt-controller;
		#interrupt-cells = <1>;
	};

	memory { device_type = "memory"; reg = <0 0>; };

	ubus@10000000 {
		#address-cells = <1>;
		#size-cells = <1>;
		ranges;
		compatible = "simple-bus";
		interrupt-parent = <&periph_intc>;

		ext_intc0: interrupt-controller@10000018 {
			compatible = "brcm,bcm6345-ext-intc";
			reg = <0x10000018 0x4>;

			interrupt-controller;
			#interrupt-cells = <2>;

			interrupts = <20>, <21>, <22>, <23>;
		};

		ext_intc1: interrupt-controller@1000001c {
			compatible = "brcm,bcm6345-ext-intc";
			reg = <0x1000001c 0x4>;

			interrupt-controller;
			#interrupt-cells = <2>;

			interrupts = <24>, <25>;
		};

		periph_intc: interrupt-controller@10000020 {
			compatible = "brcm,bcm6345-l1-intc";
			reg = <0x10000020 0x10>,
			      <0x10000030 0x10>;

			interrupt-controller;
			#interrupt-cells = <1>;

			interrupt-parent = <&cpu_intc>;
			interrupts = <2>, <3>;
		};

		pinctrl: pin-controller@10000080 {
			compatible = "brcm,bcm6368-pinctrl";
			reg = <0x10000080 0x8>,
			      <0x10000088 0x8>,
			      <0x10000098 0x4>;
			reg-names = "dirout", "dat", "mode";
			brcm,gpiobasemode = <&gpiobasemode>;

			gpio-controller;
			#gpio-cells = <2>;

			interrupts-extended = <&ext_intc1 0 0>,
					      <&ext_intc1 1 0>,
					      <&ext_intc0 0 0>,
					      <&ext_intc0 1 0>,
					      <&ext_intc0 2 0>,
					      <&ext_intc0 3 0>;
			interrupt-names = "gpio32", "gpio33", "gpio34", "gpio35",
					  "gpio36", "gpio37";

			pinctrl_analog_afe_0: analog_afe_0 {
				function = "analog_afe_0";
				pins = "gpio0";
			};

			pinctrl_analog_afe_1: analog_afe_1 {
				function = "analog_afe_1";
				pins = "gpio1";
			};

			pinctrl_sys_irq: sys_irq {
				function = "sys_irq";
				pins = "gpio2";
			};

			pinctrl_serial_led: serial_led {
				pinctrl_serial_led_data: serial_led_data {
					function = "serial_led_data";
					pins = "gpio3";
				};

				pinctrl_serial_led_clk: serial_led_clk {
					function = "serial_led_clk";
					pins = "gpio4";
				};
			};

			pinctrl_inet_led: inet_led {
				function = "inet_led";
				pins = "gpio5";
			};

			pinctrl_ephy0_led: ephy0_led {
				function = "ephy0_led";
				pins = "gpio6";
			};

			pinctrl_ephy1_led: ephy1_led {
				function = "ephy1_led";
				pins = "gpio7";
			};

			pinctrl_ephy2_led: ephy2_led {
				function = "ephy2_led";
				pins = "gpio8";
			};

			pinctrl_ephy3_led: ephy3_led {
				function = "ephy3_led";
				pins = "gpio9";
			};

			pinctrl_robosw_led_data: robosw_led_data {
				function = "robosw_led_data";
				pins = "gpio10";
			};

			pinctrl_robosw_led_clk: robosw_led_clk {
				function = "robosw_led_clk";
				pins = "gpio11";
			};

			pinctrl_robosw_led0: robosw_led0 {
				function = "robosw_led0";
				pins = "gpio12";
			};

			pinctrl_robosw_led1: robosw_led1 {
				function = "robosw_led1";
				pins = "gpio13";
			};

			pinctrl_usb_device_led: usb_device_led {
				function = "usb_device_led";
				pins = "gpio14";
			};

			pinctrl_pci: pci {
				pinctrl_pci_req1: pci_req1 {
					function = "pci_req1";
					pins = "gpio16";
				};

				pinctrl_pci_gnt1: pci_gnt1 {
					function = "pci_gnt1";
					pins = "gpio17";
				};

				pinctrl_pci_intb: pci_intb {
					function = "pci_intb";
					pins = "gpio18";
				};

				pinctrl_pci_req0: pci_req0 {
					function = "pci_req0";
					pins = "gpio19";
				};

				pinctrl_pci_gnt0: pci_gnt0 {
					function = "pci_gnt0";
					pins = "gpio20";
				};
			};

			pinctrl_pcmcia: pcmcia {
				pinctrl_pcmcia_cd1: pcmcia_cd1 {
					function = "pcmcia_cd1";
					pins = "gpio22";
				};

				pinctrl_pcmcia_cd2: pcmcia_cd2 {
					function = "pcmcia_cd2";
					pins = "gpio23";
				};

				pinctrl_pcmcia_vs1: pcmcia_vs1 {
					function = "pcmcia_vs1";
					pins = "gpio24";
				};

				pinctrl_pcmcia_vs2: pcmcia_vs2 {
					function = "pcmcia_vs2";
					pins = "gpio25";
				};
			};

			pinctrl_ebi_cs2: ebi_cs2 {
				function = "ebi_cs2";
				pins = "gpio26";
			};

			pinctrl_ebi_cs3: ebi_cs3 {
				function = "ebi_cs2";
				pins = "gpio27";
			};

			pinctrl_spi_cs2: spi_cs2 {
				function = "spi_cs2";
				pins = "gpio28";
			};

			pinctrl_spi_cs3: spi_cs3 {
				function = "spi_cs3";
				pins = "gpio29";
			};

			pinctrl_spi_cs4: spi_cs4 {
				function = "spi_cs4";
				pins = "gpio30";
			};

			pinctrl_spi_cs5: spi_cs5 {
				function = "spi_cs5";
				pins = "gpio31";
			};

			pinctrl_uart1: uart1 {
				function = "uart1";
				group = "uart1_grp";
			};
		};

		gpiobasemode: gpiobasemode@100000b8 {
			compatible = "brcm,bcm6368-gpiobasemode", "syscon";
			reg = <0x100000b8 0x4>;
		};

		leds: led-controller@100000d0 {
			#address-cells = <1>;
			#size-cells = <0>;
			compatible = "brcm,bcm6358-leds";
			reg = <0x100000d0 0x8>;
			status = "disabled";
		};

		uart0: serial@10000100 {
			compatible = "brcm,bcm6345-uart";
			reg = <0x10000100 0x18>;

			interrupt-parent = <&periph_intc>;
			interrupts = <2>;

			/* clocks = <&periph_clk>; */
			/* clock-names = "refclk"; */

			status = "disabled";
		};

		uart1: serial@10000120 {
			compatible = "brcm,bcm6345-uart";
			reg = <0x10000120 0x18>;

			interrupt-parent = <&periph_intc>;
			interrupts = <3>;

			/* clocks = <&periph_clk>; */
			/* clock-names = "refclk"; */

			status = "disabled";
		};

		nflash: nand@10000200 {
			#address-cells = <1>;
			#size-cells = <0>;
			compatible = "brcm,nand-bcm6368",
				     "brcm,brcmnand-v2.1",
				     "brcm,brcmnand";
			reg = <0x10000200 0x180>,
			      <0x10000600 0x200>,
			      <0x10000070 0x10>;
			reg-names = "nand",
				    "nand-cache",
				    "nand-int-base";

			interrupt-parent = <&periph_intc>;
			interrupts = <10>;

			/* clocks = <&clkctl 17>; */

			status = "disabled";
		};

		lsspi: spi@10000800 {
			#address-cells = <1>;
			#size-cells = <0>;
			compatible = "brcm,bcm6358-spi";
			reg = <0x10000800 0x70c>;
			interrupts = <1>;
			/* clocks = <&clkctl 9>; */
		};
	};

	pflash: nor@18000000 {
		compatible = "cfi-flash";
		reg = <0x18000000 0x2000000>;
		bank-width = <2>;
		#address-cells = <1>;
		#size-cells = <1>;
		status = "disabled";
	};
};
