From fd66cd0d79cb836badecb91fdd19afd32afbb443 Mon Sep 17 00:00:00 2001
From: Florian Fainelli <f.fainelli@gmail.com>
Date: Mon, 9 Nov 2020 12:02:08 -0800
Subject: [PATCH 13/16] ARM: dts: NSP: Update ethernet switch node name

Update the switch unit name from srab to ethernet-switch, allowing us
to fix warnings such as:

     CHECK   arch/arm/boot/dts/bcm4708-buffalo-wzr-1750dhp.dt.yaml
    arch/arm/boot/dts/bcm4708-buffalo-wzr-1750dhp.dt.yaml:
    srab@18007000: $nodename:0: 'srab@18007000' does not match
    '^(ethernet-)?switch(@.*)?$'
            From schema:
    Documentation/devicetree/bindings/net/dsa/b53.yaml

Reviewed-by: Vladimir Oltean <olteanv@gmail.com>
Signed-off-by: Florian Fainelli <f.fainelli@gmail.com>
---
 arch/arm/boot/dts/bcm-nsp.dtsi | 2 +-
 1 file changed, 1 insertion(+), 1 deletion(-)

--- a/arch/arm/boot/dts/bcm-nsp.dtsi
+++ b/arch/arm/boot/dts/bcm-nsp.dtsi
@@ -385,7 +385,7 @@
 			clock-names = "apb_pclk";
 		};
 
-		srab: srab@36000 {
+		srab: ethernet-switch@36000 {
 			compatible = "brcm,nsp-srab";
 			reg = <0x36000 0x1000>,
 			      <0x3f308 0x8>,
