From 81bb218c829246962a6327c64eec18ddcc049936 Mon Sep 17 00:00:00 2001
From: Hauke Mehrtens <hauke@hauke-m.de>
Date: Sun, 18 Apr 2021 23:46:16 +0200
Subject: mtd: parsers: trx: Allow to use TRX parser on Mediatek SoCs

Buffalo uses the TRX partition format also on Mediatek MT7622 SoCs.

Signed-off-by: Hauke Mehrtens <hauke@hauke-m.de>
Signed-off-by: Miquel Raynal <miquel.raynal@bootlin.com>
Link: https://lore.kernel.org/linux-mtd/20210418214616.239574-4-hauke@hauke-m.de
---
 drivers/mtd/parsers/Kconfig | 2 +-
 1 file changed, 1 insertion(+), 1 deletion(-)

--- a/drivers/mtd/parsers/Kconfig
+++ b/drivers/mtd/parsers/Kconfig
@@ -131,7 +131,7 @@ config MTD_AFS_PARTS
 
 config MTD_PARSER_TRX
 	tristate "Parser for TRX format partitions"
-	depends on MTD && (BCM47XX || ARCH_BCM_5301X || COMPILE_TEST)
+	depends on MTD && (BCM47XX || ARCH_BCM_5301X || ARCH_MEDIATEK || COMPILE_TEST)
 	help
 	  TRX is a firmware format used by Broadcom on their devices. It
 	  may contain up to 3/4 partitions (depending on the version).
