From 0bf118ac01f74d16e6220261b0ca66928587fb43 Mon Sep 17 00:00:00 2001
From: Dom Cobley <popcornmix@gmail.com>
Date: Mon, 22 Feb 2021 18:47:19 +0000
Subject: [PATCH] clk-raspberrypi: Also support HEVC clock

Signed-off-by: Dom Cobley <popcornmix@gmail.com>
---
 drivers/clk/bcm/clk-raspberrypi.c | 1 +
 1 file changed, 1 insertion(+)

--- a/drivers/clk/bcm/clk-raspberrypi.c
+++ b/drivers/clk/bcm/clk-raspberrypi.c
@@ -271,6 +271,7 @@ static int raspberrypi_discover_clocks(s
 		case RPI_FIRMWARE_CORE_CLK_ID:
 		case RPI_FIRMWARE_M2MC_CLK_ID:
 		case RPI_FIRMWARE_V3D_CLK_ID:
+		case RPI_FIRMWARE_HEVC_CLK_ID:
 		case RPI_FIRMWARE_PIXEL_BVB_CLK_ID:
 			hw = raspberrypi_clk_register(rpi, clks->parent,
 						      clks->id);
