From c90422ce5c24b9f1f4c03e935918e85bef6cb336 Mon Sep 17 00:00:00 2001
From: Ahmet Inan <inan@aicodix.de>
Date: Wed, 4 Aug 2021 10:10:11 +0200
Subject: [PATCH] Revert "overlays: Update display GPIO declarations"
 for Goodix

This reverts commit b7d685c0b1bd1b98af0e9c1f5d43769982bdbfb2 for Goodix

Signed-off-by: Ahmet Inan <inan@aicodix.de>
---
 arch/arm/boot/dts/overlays/goodix-overlay.dts | 2 +-
 1 file changed, 1 insertion(+), 1 deletion(-)

--- a/arch/arm/boot/dts/overlays/goodix-overlay.dts
+++ b/arch/arm/boot/dts/overlays/goodix-overlay.dts
@@ -31,7 +31,7 @@
 				interrupt-parent = <&gpio>;
 				interrupts = <4 2>; // high-to-low edge triggered
 				irq-gpios = <&gpio 4 0>; // Pin7 on GPIO header
-				reset-gpios = <&gpio 17 1>; // Pin11 on GPIO header
+				reset-gpios = <&gpio 17 0>; // Pin11 on GPIO header
 			};
 		};
 	};
