From 3c1991fe18bca459d07dd78a2268e26008707f00 Mon Sep 17 00:00:00 2001
From: Ran Wang <ran.wang_1@nxp.com>
Date: Mon, 25 Feb 2019 13:38:01 +0800
Subject: [PATCH] ARM: dts: Fix DWC3 IP VBUS glitch issue on LS1021A

Signed-off-by: Ran Wang <ran.wang_1@nxp.com>
---
 arch/arm/boot/dts/ls1021a.dtsi | 1 +
 1 file changed, 1 insertion(+)

--- a/arch/arm/boot/dts/ls1021a.dtsi
+++ b/arch/arm/boot/dts/ls1021a.dtsi
@@ -877,6 +877,7 @@
 			usb3-lpm-capable;
 			snps,dis-u1u2-when-u3-quirk;
 			snps,incr-burst-type-adjustment = <1>, <4>, <8>, <16>;
+			snps,host-vbus-glitches;
 		};
 
 		pcie@3400000 {
