From 6c3655acaa5766efe81f60ac6d428b0d184daa0d Mon Sep 17 00:00:00 2001
From: Yinbo Zhu <yinbo.zhu@nxp.com>
Date: Fri, 21 Dec 2018 11:38:44 +0800
Subject: [PATCH] ARM: dts: ls1021aqds: enable esdhc controller

This patch is to enable esdhc controller in ls1021aqds

Signed-off-by: Yinbo Zhu <yinbo.zhu@nxp.com>
---
 arch/arm/boot/dts/ls1021a-qds.dts | 4 ++++
 1 file changed, 4 insertions(+)

--- a/arch/arm/boot/dts/ls1021a-qds.dts
+++ b/arch/arm/boot/dts/ls1021a-qds.dts
@@ -165,6 +165,10 @@
 	status = "okay";
 };
 
+&esdhc {
+	status = "okay";
+};
+
 &i2c0 {
 	status = "okay";
 
